# Function u32x4_relaxed_dot_i8x16_i7x16_add

Source

    pub fn u32x4_relaxed_dot_i8x16_i7x16_add(a: v128, b: v128, c: v128) -> v128

🔬This is a nightly-only experimental API. (`simd_wasm64` #90599)
Available on `target_family="wasm"` and target feature `relaxed-simd` and WebAssembly only.
Expand description

Similar to `i16x8_relaxed_dot_i8x16_i7x16` except that the intermediate `i16x8` result is fed into `i32x4_extadd_pairwise_i16x8` followed by `i32x4_add` to add the value `c` to the result.