# Function _mm_load_pd

1.27.0 · Source

    pub unsafe fn _mm_load_pd(mem_addr: *const f64) -> __m128d

Available on (x86 or x86-64) and target feature `sse2` and x86 only.
Expand description

Loads 128-bits (composed of 2 packed double-precision (64-bit) floating-point elements) from memory into the returned vector. `mem_addr` must be aligned on a 16-byte boundary or a general-protection exception may be generated.

Intel’s documentation