# Function _mm512_maskz_cvtepu32_pd

1.89.0 · Source

    pub fn _mm512_maskz_cvtepu32_pd(k: __mmask8, a: __m256i) -> __m512d

Available on (x86 or x86-64) and target feature `avx512f` and x86-64 only.
Expand description

Convert packed unsigned 32-bit integers in a to packed double-precision (64-bit) floating-point elements, and store the results in dst using zeromask k (elements are zeroed out when the corresponding mask bit is not set).

Intel’s documentation