# Function _mm512_maskz_fnmsub_pd

1.89.0 · Source

    pub fn _mm512_maskz_fnmsub_pd(
        k: __mmask8,
        a: __m512d,
        b: __m512d,
        c: __m512d,
    ) -> __m512d

Available on (x86 or x86-64) and target feature `avx512f` and x86-64 only.
Expand description

Multiply packed double-precision (64-bit) floating-point elements in a and b, subtract packed elements in c from the negated intermediate result, and store the results in dst using zeromask k (elements are zeroed out when the corresponding mask bit is not set).

Intel’s documentation