n <linmq006@gmail.com>
---
 drivers/dma/qcom/gpi.c | 6 ++++--
 1 file changed, 4 insertions(+), 2 deletions(-)

diff --git a/drivers/dma/qcom/gpi.c b/drivers/dma/qcom/gpi.c
index 8e87738086b2..8908b7c71900 100644
--- a/drivers/dma/qcom/gpi.c
+++ b/drivers/dma/qcom/gpi.c
@@ -1605,14 +1605,16 @@ static int
 gpi_peripheral_config(struct dma_chan *chan, struct dma_slave_config *config)
 {
 	struct gchan *gchan = to_gchan(chan);
+	void *new_config;
 
 	if (!config->peripheral_config)
 		return -EINVAL;
 
-	gchan->config = krealloc(gchan->config, config->peripheral_size, GFP_NOWAIT);
-	if (!gchan->config)
+	new_config = krealloc(gchan->config, config->peripheral_size, GFP_NOWAIT);
+	if (!new_config)
 		return -ENOMEM;
 
+	gchan->config = new_config;
 	memcpy(gchan->config, config->peripheral_config, config->peripheral_size);
 
 	return 0;
-- 
2.39.5 (Apple Git-154)[PATCH] dma: qcom: gpi: Fix memory leak in gpi_peripheral_config()Miaoqian Lin <linmq006@gmail.com> undefinedVinod Koul <vkoul@kernel.org>, Neil Armstrong <neil.armstrong@linaro.org>, Jyothi Kumar Seerapu <quic_jseerapu@quicinc.com>, Krzysztof Kozlowski <krzysztof.kozlowski@linaro.org>, Dmitry Baryshkov <lumag@kernel.org>, linux-arm-msm@vger.kernel.org, dmaengine@vger.kernel.org, linux-kernel@vger.kernel.org undefined undefined undefined undefined undefined undefined undefined undefined undefinedƒ,ƒÜ?	