Home Features Getting Started Mailing List / Help Contribute Protocols VPN Server

OpenConnect VPN client

Feature list Running as non-root user GUI Character sets One Time Passwords Smart Cards / PKCS#11 Trusted Platform Module (TPM) Cisco Secure Desktop (CSD) Juniper Host Checker (TNCC) Host Integrity Protection (HIP)

# Features

- Connection through HTTP proxy, including libproxy support for automatic proxy configuration.
- Connection through SOCKS5 proxy.
- Automatic detection of IPv4 and IPv6 address, routes.
- Authentication via HTTP forms.
- Authentication using SSL certificates — from local file, Trusted Platform Module and PKCS#11 smartcards.
- Authentication using SecurID software tokens (when built with libstoken)
- Authentication using OATH TOTP or HOTP software tokens.
- Authentication using Yubikey OATH tokens (when built with libpcsclite)
- UserGroup support for selecting between multiple configurations on a single VPN server.
- Data transport over TCP (HTTPS) or UDP (DTLS or ESP).
- Keepalive and Dead Peer Detection on both HTTPS and DTLS.
- Automatic update of VPN server list / configuration.
- Roaming support, allowing reconnection when the local IP address changes.
- Run without root privileges (see here).
- Support for "Cisco Secure Desktop" (see here), Juniper TNCC (see here), and "GlobalProtect HIP report" (see here).
- Graphical connection tools for various environments (see here).