# Function _mm_testn_epi64_mask

1.89.0 · Source

    pub fn _mm_testn_epi64_mask(a: __m128i, b: __m128i) -> __mmask8

Available on (x86 or x86-64) and target feature `avx512f` and target feature `avx512vl` and x86 only.
Expand description

Compute the bitwise NAND of packed 64-bit integers in a and b, producing intermediate 64-bit values, and set the corresponding bit in result mask k if the intermediate value is zero.

Intel’s documentation