{
  "schema_version": "1.4.0",
  "id": "GHSA-5f23-7wg5-v6qm",
  "modified": "2025-04-20T03:41:22Z",
  "published": "2022-05-14T02:49:20Z",
  "aliases": [
    "CVE-2015-2279"
  ],
  "details": "cgi_test.cgi in AirLive BU-2015 with firmware 1.03.18, BU-3026 with firmware 1.43, and MD-3025 with firmware 1.81 allows remote attackers to execute arbitrary OS commands via shell metacharacters after an \"&\" (ampersand) in the write_mac write_pid, write_msn, write_tan, or write_hdv parameter.",
  "severity": [
    {
      "type": "CVSS_V3",
      "score": "CVSS:3.0/AV:N/AC:L/PR:N/UI:N/S:U/C:H/I:H/A:H"
    }
  ],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2015-2279"
    },
    {
      "type": "WEB",
      "url": "https://www.coresecurity.com/advisories/airlive-multiple-products-os-command-injection"
    },
    {
      "type": "WEB",
      "url": "https://www.exploit-db.com/exploits/37532"
    },
    {
      "type": "WEB",
      "url": "http://packetstormsecurity.com/files/132585/AirLive-Remote-Command-Injection.html"
    },
    {
      "type": "WEB",
      "url": "http://seclists.org/fulldisclosure/2015/Jul/29"
    },
    {
      "type": "WEB",
      "url": "http://www.securityfocus.com/archive/1/535938/100/0/threaded"
    },
    {
      "type": "WEB",
      "url": "http://www.securityfocus.com/bid/75559"
    }
  ],
  "database_specific": {
    "cwe_ids": [
      "CWE-78"
    ],
    "severity": "CRITICAL",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2017-07-25T01:29:00Z"
  }
}