{
  "schema_version": "1.4.0",
  "id": "GHSA-7qw8-4g2g-2m86",
  "modified": "2022-05-13T01:28:35Z",
  "published": "2022-05-13T01:28:35Z",
  "aliases": [
    "CVE-2013-5709"
  ],
  "details": "The authentication implementation in the web server on Siemens SCALANCE X-200 switches with firmware before 5.0.0 does not use a sufficient source of entropy for generating values of random numbers, which makes it easier for remote attackers to hijack sessions by predicting a value.",
  "severity": [],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2013-5709"
    },
    {
      "type": "WEB",
      "url": "https://cert-portal.siemens.com/productcert/pdf/ssa-850708.pdf"
    },
    {
      "type": "WEB",
      "url": "http://ics-cert.us-cert.gov/advisories/ICSA-13-254-01"
    },
    {
      "type": "WEB",
      "url": "http://www.siemens.com/corporate-technology/pool/de/forschungsfelder/siemens_security_advisory_ssa-850708.pdf"
    }
  ],
  "database_specific": {
    "cwe_ids": [],
    "severity": "HIGH",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2013-09-17T12:04:00Z"
  }
}