{
  "schema_version": "1.4.0",
  "id": "GHSA-f446-wm48-q9x7",
  "modified": "2025-04-11T04:05:00Z",
  "published": "2022-05-17T01:42:17Z",
  "aliases": [
    "CVE-2012-4366"
  ],
  "details": "Belkin wireless routers Surf N150 Model F7D1301v1, N900 Model F9K1104v1, N450 Model F9K1105V2, and N300 Model F7D2301v1 generate a predictable default WPA2-PSK passphrase based on eight digits of the WAN MAC address, which allows remote attackers to access the network by sniffing the beacon frames.",
  "severity": [],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2012-4366"
    },
    {
      "type": "WEB",
      "url": "https://exchange.xforce.ibmcloud.com/vulnerabilities/80157"
    },
    {
      "type": "WEB",
      "url": "http://archives.neohapsis.com/archives/bugtraq/2012-11/0070.html"
    },
    {
      "type": "WEB",
      "url": "http://www.jakoblell.com/blog/2012/11/19/cve-2012-4366-insecure-default-wpa2-passphrase-in-multiple-belkin-wireless-routers"
    },
    {
      "type": "WEB",
      "url": "http://www.securityfocus.com/bid/56591"
    }
  ],
  "database_specific": {
    "cwe_ids": [],
    "severity": "LOW",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2012-11-20T00:55:00Z"
  }
}