{
  "schema_version": "1.4.0",
  "id": "GHSA-g3f4-c293-32x8",
  "modified": "2022-05-17T00:12:50Z",
  "published": "2022-05-17T00:12:50Z",
  "aliases": [
    "CVE-2012-1806"
  ],
  "details": "The ECOM Ethernet module in Koyo H0-ECOM, H0-ECOM100, H2-ECOM, H2-ECOM-F, H2-ECOM100, H4-ECOM, H4-ECOM-F, and H4-ECOM100 supports a maximum password length of 8 bytes, which makes it easier for remote attackers to obtain access via a brute-force attack.",
  "severity": [],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2012-1806"
    },
    {
      "type": "WEB",
      "url": "https://exchange.xforce.ibmcloud.com/vulnerabilities/74876"
    },
    {
      "type": "WEB",
      "url": "http://www.us-cert.gov/control_systems/pdf/ICSA-12-102-02.pdf"
    }
  ],
  "database_specific": {
    "cwe_ids": [
      "CWE-287"
    ],
    "severity": "HIGH",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2012-04-13T17:55:00Z"
  }
}