{
  "schema_version": "1.4.0",
  "id": "GHSA-ffqg-m22j-5p83",
  "modified": "2022-05-24T17:09:10Z",
  "published": "2022-05-24T17:09:10Z",
  "aliases": [
    "CVE-2020-5531"
  ],
  "details": "Mitsubishi Electric MELSEC C Controller Module and MELIPC Series MI5000 MELSEC-Q Series C Controller Module(Q24DHCCPU-V, Q24DHCCPU-VG User Ethernet port (CH1, CH2): First 5 digits of serial number 21121 or before), MELSEC iQ-R Series C Controller Module / C Intelligent Function Module(R12CCPU-V Ethernet port (CH1, CH2): First 2 digits of serial number 11 or before, and RD55UP06-V Ethernet port: First 2 digits of serial number 08 or before), and MELIPC Series MI5000(MI5122-VW Ethernet port (CH1): First 2 digits of serial number 03 or before, or the firmware version 03 or before) allow remote attackers to cause a denial of service and/or malware being executed via unspecified vectors.",
  "severity": [],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2020-5531"
    },
    {
      "type": "WEB",
      "url": "https://jvn.jp/en/vu/JVNVU95424547/index.html"
    },
    {
      "type": "WEB",
      "url": "https://www.mitsubishielectric.com/en/psirt/vulnerability/pdf/2019-003_en.pdf"
    }
  ],
  "database_specific": {
    "cwe_ids": [],
    "severity": "HIGH",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2020-02-17T07:15:00Z"
  }
}