{
  "schema_version": "1.4.0",
  "id": "GHSA-hc22-58vm-mg54",
  "modified": "2022-05-13T01:28:30Z",
  "published": "2022-05-13T01:28:30Z",
  "aliases": [
    "CVE-2013-2805"
  ],
  "details": "Rockwell Automation RSLinx Enterprise Software (LogReceiver.exe) CPR9, CPR9-SR1, CPR9-SR2, CPR9-SR3, CPR9-SR4, CPR9-SR5, CPR9-SR5.1, and CPR9-SR6 does not handle input correctly and results in a logic error if it receives a datagram with an incorrect value in the “Record Data Size” field. By sending a datagram to the service over Port 4444/UDP with the “Record Data Size” field modified to an oversized value, an attacker could cause an out-of-bounds read access violation that leads to a service crash. The service can be recovered with a manual reboot. The patches and details pertaining to this vulnerability can be found at the following Rockwell Automation Security Advisory link (login is required): https://rockwellautomation.custhelp.com/app/answers/detail/a_id/537599",
  "severity": [
    {
      "type": "CVSS_V3",
      "score": "CVSS:3.0/AV:N/AC:L/PR:N/UI:N/S:U/C:N/I:N/A:H"
    }
  ],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2013-2805"
    },
    {
      "type": "WEB",
      "url": "https://ics-cert.us-cert.gov/advisories/ICSA-13-095-02"
    }
  ],
  "database_specific": {
    "cwe_ids": [
      "CWE-125"
    ],
    "severity": "HIGH",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2019-03-26T18:29:00Z"
  }
}