{
  "schema_version": "1.4.0",
  "id": "GHSA-qj75-j4wq-j748",
  "modified": "2022-08-18T00:00:18Z",
  "published": "2022-08-11T00:00:22Z",
  "aliases": [
    "CVE-2022-36323"
  ],
  "details": "A vulnerability has been identified in SCALANCE M-800 / S615 (All versions), SCALANCE SC-600 family (All versions < V2.3.1), SCALANCE W-1700 IEEE 802.11ac family (All versions), SCALANCE W-700 IEEE 802.11ax family (All versions), SCALANCE W-700 IEEE 802.11n family (All versions), SCALANCE XB-200 switch family (All versions), SCALANCE XC-200 switch family (All versions), SCALANCE XF-200BA switch family (All versions), SCALANCE XM-400 Family (All versions), SCALANCE XP-200 switch family (All versions), SCALANCE XR-300WG switch family (All versions), SCALANCE XR-500 Family (All versions). Affected devices do not properly sanitize an input field. This could allow an authenticated remote attacker with administrative privileges to inject code or spawn a system root shell.",
  "severity": [
    {
      "type": "CVSS_V3",
      "score": "CVSS:3.1/AV:N/AC:L/PR:H/UI:N/S:U/C:H/I:H/A:H"
    }
  ],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2022-36323"
    },
    {
      "type": "WEB",
      "url": "https://cert-portal.siemens.com/productcert/pdf/ssa-710008.pdf"
    }
  ],
  "database_specific": {
    "cwe_ids": [
      "CWE-74"
    ],
    "severity": "HIGH",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2022-08-10T12:15:00Z"
  }
}