{
  "schema_version": "1.4.0",
  "id": "GHSA-jqrp-j828-97gh",
  "modified": "2022-05-13T01:31:44Z",
  "published": "2022-05-13T01:31:44Z",
  "aliases": [
    "CVE-2018-8869"
  ],
  "details": "In Lantech IDS 2102 2.0 and prior, nearly all input fields allow for arbitrary input on the device. A CVSS v3 base score of 9.8 has been calculated; the CVSS vector string is (AV:N/AC:L/PR:N/UI:N/S:U/C:H/I:H/A:H).",
  "severity": [
    {
      "type": "CVSS_V3",
      "score": "CVSS:3.0/AV:N/AC:L/PR:N/UI:N/S:U/C:H/I:H/A:H"
    }
  ],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2018-8869"
    },
    {
      "type": "WEB",
      "url": "https://ics-cert.us-cert.gov/advisories/ICSA-18-123-01"
    },
    {
      "type": "WEB",
      "url": "http://www.securityfocus.com/bid/104098"
    }
  ],
  "database_specific": {
    "cwe_ids": [
      "CWE-20"
    ],
    "severity": "CRITICAL",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2018-05-04T17:29:00Z"
  }
}