{
  "schema_version": "1.4.0",
  "id": "GHSA-jwv4-wwvg-5p94",
  "modified": "2022-05-13T01:34:41Z",
  "published": "2022-05-13T01:34:41Z",
  "aliases": [
    "CVE-2018-13815"
  ],
  "details": "A vulnerability has been identified in SIMATIC S7-1200 (All versions), SIMATIC S7-1500 (All Versions < V2.6). An attacker could exhaust the available connection pool of an affected device by opening a sufficient number of connections to the device. Successful exploitation requires an attacker to be able to send packets to port 102/tcp of the affected device. No user interaction and no user privileges are required to exploit the vulnerability. The vulnerability, if exploited, could cause a Denial-of-Service condition impacting the availability of the system. At the time of advisory publication no public exploitation of this vulnerability was known.",
  "severity": [
    {
      "type": "CVSS_V3",
      "score": "CVSS:3.0/AV:N/AC:L/PR:N/UI:N/S:U/C:N/I:N/A:H"
    }
  ],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2018-13815"
    },
    {
      "type": "WEB",
      "url": "https://cert-portal.siemens.com/productcert/pdf/ssa-584286.pdf"
    },
    {
      "type": "WEB",
      "url": "http://www.securityfocus.com/bid/105928"
    }
  ],
  "database_specific": {
    "cwe_ids": [
      "CWE-400"
    ],
    "severity": "HIGH",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2018-12-13T16:29:00Z"
  }
}