{
  "schema_version": "1.4.0",
  "id": "GHSA-jxqj-hhh8-m26w",
  "modified": "2022-05-17T05:28:35Z",
  "published": "2022-05-17T05:28:35Z",
  "aliases": [
    "CVE-2011-2561"
  ],
  "details": "The SIP process in Cisco Unified Communications Manager (aka CUCM, formerly CallManager) 7.x before 7.1(5b)su4 and 8.x before 8.0(1) does not properly handle SDP data within a SIP call in certain situations related to use of the g729ar8 codec for a Media Termination Point (MTP), which allows remote attackers to cause a denial of service (service outage) via a crafted call, aka Bug ID CSCtc61990.",
  "severity": [],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2011-2561"
    },
    {
      "type": "WEB",
      "url": "http://www.cisco.com/en/US/products/products_security_advisory09186a0080b8f531.shtml"
    }
  ],
  "database_specific": {
    "cwe_ids": [],
    "severity": "HIGH",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2011-08-29T15:55:00Z"
  }
}