{
  "schema_version": "1.4.0",
  "id": "GHSA-m5fq-q49w-wc2j",
  "modified": "2022-05-24T19:07:20Z",
  "published": "2022-05-24T19:07:20Z",
  "aliases": [
    "CVE-2021-33012"
  ],
  "details": "Rockwell Automation MicroLogix 1100, all versions, allows a remote, unauthenticated attacker sending specially crafted commands to cause the PLC to fault when the controller is switched to RUN mode, which results in a denial-of-service condition. If successfully exploited, this vulnerability will cause the controller to fault whenever the controller is switched to RUN mode.",
  "severity": [],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2021-33012"
    },
    {
      "type": "WEB",
      "url": "https://us-cert.cisa.gov/ics/advisories/icsa-21-189-01"
    }
  ],
  "database_specific": {
    "cwe_ids": [],
    "severity": "HIGH",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2021-07-09T15:15:00Z"
  }
}