{
  "schema_version": "1.4.0",
  "id": "GHSA-m6xr-cgmm-vx52",
  "modified": "2022-05-13T01:35:01Z",
  "published": "2022-05-13T01:35:01Z",
  "aliases": [
    "CVE-2018-10592"
  ],
  "details": "Yokogawa STARDOM FCJ controllers R4.02 and prior, FCN-100 controllers R4.02 and prior, FCN-RTU controllers R4.02 and prior, and FCN-500 controllers R4.02 and prior utilize hard-coded credentials that could allow an attacker to gain unauthorized administrative access to the device, which could result in remote code execution.",
  "severity": [
    {
      "type": "CVSS_V3",
      "score": "CVSS:3.0/AV:N/AC:L/PR:N/UI:N/S:U/C:H/I:H/A:H"
    }
  ],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2018-10592"
    },
    {
      "type": "WEB",
      "url": "https://ics-cert.us-cert.gov/advisories/ICSA-18-151-03"
    },
    {
      "type": "WEB",
      "url": "https://web-material3.yokogawa.com/1/6712/details/YSAR-18-0004-E.pdf"
    },
    {
      "type": "WEB",
      "url": "http://www.securityfocus.com/bid/104376"
    }
  ],
  "database_specific": {
    "cwe_ids": [
      "CWE-798"
    ],
    "severity": "CRITICAL",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2018-07-31T17:29:00Z"
  }
}