{
  "schema_version": "1.4.0",
  "id": "GHSA-m6hh-6w6m-5h5c",
  "modified": "2022-05-24T19:14:29Z",
  "published": "2022-05-24T19:14:29Z",
  "aliases": [
    "CVE-2021-37206"
  ],
  "details": "A vulnerability has been identified in SIPROTEC 5 relays with CPU variants CP050 (All versions < V8.80), SIPROTEC 5 relays with CPU variants CP100 (All versions < V8.80), SIPROTEC 5 relays with CPU variants CP200 (All versions < V8.80), SIPROTEC 5 relays with CPU variants CP300 (All versions < V8.80). Received webpackets are not properly processed. An unauthenticated remote attacker with access to any of the Ethernet interfaces could send specially crafted packets to force a restart of the target device.",
  "severity": [],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2021-37206"
    },
    {
      "type": "WEB",
      "url": "https://cert-portal.siemens.com/productcert/pdf/ssa-500748.pdf"
    }
  ],
  "database_specific": {
    "cwe_ids": [
      "CWE-20"
    ],
    "severity": "HIGH",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2021-09-14T11:15:00Z"
  }
}