{
  "schema_version": "1.4.0",
  "id": "GHSA-mp5j-gcgv-qr44",
  "modified": "2022-05-21T00:00:51Z",
  "published": "2022-05-12T00:00:40Z",
  "aliases": [
    "CVE-2021-33317"
  ],
  "details": "The TRENDnet TI-PG1284i switch(hw v2.0R) prior to version 2.0.2.S0 suffers from a null pointer dereference vulnerability. This vulnerability exists in its lldp related component. Due to fail to check if ChassisID TLV is contained in the packet, by sending a crafted lldp packet to the device, an attacker can crash the process due to null pointer dereference.",
  "severity": [
    {
      "type": "CVSS_V3",
      "score": "CVSS:3.1/AV:N/AC:L/PR:N/UI:N/S:U/C:N/I:N/A:H"
    }
  ],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2021-33317"
    },
    {
      "type": "WEB",
      "url": "https://www.trendnet.com/support/view.asp?cat=4&id=81"
    }
  ],
  "database_specific": {
    "cwe_ids": [
      "CWE-476"
    ],
    "severity": "HIGH",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2022-05-11T18:15:00Z"
  }
}