{
  "schema_version": "1.4.0",
  "id": "GHSA-98hm-c56g-vjqc",
  "modified": "2024-04-04T04:17:06Z",
  "published": "2023-05-23T00:30:15Z",
  "aliases": [
    "CVE-2022-47311"
  ],
  "details": "A proprietary protocol for iBoot devices is used for control and keepalive commands. The function compares the username and password; it also contains the configuration data for the user specified. If the user does not exist, then it sends a value for username and password, which allows successful authentication for a connection.",
  "severity": [
    {
      "type": "CVSS_V3",
      "score": "CVSS:3.1/AV:N/AC:L/PR:L/UI:N/S:C/C:H/I:L/A:N"
    }
  ],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2022-47311"
    },
    {
      "type": "WEB",
      "url": "https://dataprobe.com/support/iboot-pdu/local_upgrade_pdu_procedure.pdf"
    },
    {
      "type": "WEB",
      "url": "https://www.cisa.gov/news-events/ics-advisories/icsa-22-263-03"
    }
  ],
  "database_specific": {
    "cwe_ids": [
      "CWE-288"
    ],
    "severity": "HIGH",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2023-05-22T23:15:09Z"
  }
}