#
#  Arduino Zero OpenOCD script.
#
#  Copyright (c) 2014-2015 Arduino LLC.  All right reserved.
#
#  This library is free software; you can redistribute it and/or
#  modify it under the terms of the GNU Lesser General Public
#  License as published by the Free Software Foundation; either
#  version 2.1 of the License, or (at your option) any later version.
#
#  This library is distributed in the hope that it will be useful,
#  but WITHOUT ANY WARRANTY; without even the implied warranty of
#  MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.
#  See the GNU Lesser General Public License for more details.
#
#  You should have received a copy of the GNU Lesser General Public
#  License along with this library; if not, write to the Free Software
#  Foundation, Inc., 51 Franklin St, Fifth Floor, Boston, MA  02110-1301  USA
#

source [find interface/cmsis-dap.cfg]

# chip name
set CHIPNAME at91samd21g18
set ENDIAN little

# choose a port here
set telnet_port 0

source [find target/at91samdXX.cfg]
