[
    {
        "BriefDescription": "Clockticks for CMS units attached to CHA",
        "Counter": "0,1,2,3",
        "EventCode": "0x01",
        "EventName": "UNC_CHACMS_CLOCKTICKS",
        "PerPkg": "1",
        "PortMask": "0x000",
        "Unit": "CHACMS"
    },
    {
        "BriefDescription": "Counts the number of cycles FAST trigger is received from the global FAST distress wire.",
        "Counter": "0,1,2,3",
        "EventCode": "0x34",
        "EventName": "UNC_CHACMS_RING_SRC_THRTL",
        "Experimental": "1",
        "PerPkg": "1",
        "PortMask": "0x000",
        "Unit": "CHACMS"
    },
    {
        "BriefDescription": "Number of CHA clock cycles while the event is enabled",
        "Counter": "0,1,2,3",
        "EventCode": "0x01",
        "EventName": "UNC_CHA_CLOCKTICKS",
        "PerPkg": "1",
        "PublicDescription": "Clockticks of the uncore caching and home agent (CHA)",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "Distress signal assertion for dynamic prefetch throttle (DPT).  Threshold for distress signal assertion reached in TOR or IRQ (immediate cause for triggering).",
        "Counter": "0,1,2,3",
        "EventCode": "0x59",
        "EventName": "UNC_CHA_DISTRESS_ASSERTED.DPT_ANY",
        "PerPkg": "1",
        "PortMask": "0x000",
        "UMask": "0x3",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "Distress signal assertion for dynamic prefetch throttle (DPT).  Threshold for distress signal assertion reached in IRQ (immediate cause for triggering).",
        "Counter": "0,1,2,3",
        "EventCode": "0x59",
        "EventName": "UNC_CHA_DISTRESS_ASSERTED.DPT_IRQ",
        "PerPkg": "1",
        "UMask": "0x1",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "Distress signal assertion for dynamic prefetch throttle (DPT).  Threshold for distress signal assertion reached in TOR (immediate cause for triggering).",
        "Counter": "0,1,2,3",
        "EventCode": "0x59",
        "EventName": "UNC_CHA_DISTRESS_ASSERTED.DPT_TOR",
        "PerPkg": "1",
        "UMask": "0x2",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "Counts when a normal (Non-Isochronous) full line write is issued from the CHA to the any of the memory controller channels.",
        "Counter": "0,1,2,3",
        "EventCode": "0x5b",
        "EventName": "UNC_CHA_IMC_WRITES_COUNT.FULL",
        "Experimental": "1",
        "PerPkg": "1",
        "UMask": "0x1",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "CHA to iMC Full Line Writes Issued : ISOCH Full Line : Counts the total number of full line writes issued from the HA into the memory controller.",
        "Counter": "0,1,2,3",
        "EventCode": "0x5b",
        "EventName": "UNC_CHA_IMC_WRITES_COUNT.FULL_PRIORITY",
        "Experimental": "1",
        "PerPkg": "1",
        "UMask": "0x4",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "CHA to iMC Full Line Writes Issued : Partial Non-ISOCH : Counts the total number of full line writes issued from the HA into the memory controller.",
        "Counter": "0,1,2,3",
        "EventCode": "0x5b",
        "EventName": "UNC_CHA_IMC_WRITES_COUNT.PARTIAL",
        "Experimental": "1",
        "PerPkg": "1",
        "UMask": "0x2",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "CHA to iMC Full Line Writes Issued : ISOCH Partial : Counts the total number of full line writes issued from the HA into the memory controller.",
        "Counter": "0,1,2,3",
        "EventCode": "0x5b",
        "EventName": "UNC_CHA_IMC_WRITES_COUNT.PARTIAL_PRIORITY",
        "Experimental": "1",
        "PerPkg": "1",
        "UMask": "0x8",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "Cache Lookups: CRd Requests",
        "Counter": "0,1,2,3",
        "EventCode": "0x34",
        "EventName": "UNC_CHA_LLC_LOOKUP.CODE",
        "Experimental": "1",
        "PerPkg": "1",
        "PublicDescription": "Cache Lookups : CRd Requests",
        "UMask": "0x1bd0ff",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "Cache Lookups: Read Requests and Read Prefetches",
        "Counter": "0,1,2,3",
        "EventCode": "0x34",
        "EventName": "UNC_CHA_LLC_LOOKUP.DATA_RD",
        "Experimental": "1",
        "PerPkg": "1",
        "PublicDescription": "Counts the number of times the LLC was accessed - this includes code, data, prefetches and hints coming from L2.  This has numerous filters available.  Note the non-standard filtering equation.  This event will count requests that lookup the cache multiple times with multiple increments.  One must ALWAYS set umask bit 0 and select a state or states to match.  Otherwise, the event will count nothing.   CHAFilter0[24:21,17] bits correspond to [FMESI] state. Read transactions",
        "UMask": "0x1bc1ff",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "Cache Lookups: Read Requests, Read Prefetches, and Snoops",
        "Counter": "0,1,2,3",
        "EventCode": "0x34",
        "EventName": "UNC_CHA_LLC_LOOKUP.DATA_READ_ALL",
        "Experimental": "1",
        "PerPkg": "1",
        "PublicDescription": "Cache Lookups : Data Reads",
        "UMask": "0x1fc1ff",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "Cache Lookups: Read Requests to Locally Homed Memory",
        "Counter": "0,1,2,3",
        "EventCode": "0x34",
        "EventName": "UNC_CHA_LLC_LOOKUP.DATA_READ_LOCAL",
        "Experimental": "1",
        "PerPkg": "1",
        "PublicDescription": "Cache Lookups : Demand Data Reads, Core and LLC prefetches",
        "UMask": "0x841ff",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "Cache Lookups: Read Requests, Read Prefetches, and Snoops which miss the Cache",
        "Counter": "0,1,2,3",
        "EventCode": "0x34",
        "EventName": "UNC_CHA_LLC_LOOKUP.DATA_READ_MISS",
        "Experimental": "1",
        "PerPkg": "1",
        "PublicDescription": "Cache Lookups : Data Read Misses",
        "UMask": "0x1fc101",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "Cache Lookups: All Requests to Locally Homed Memory",
        "Counter": "0,1,2,3",
        "EventCode": "0x34",
        "EventName": "UNC_CHA_LLC_LOOKUP.LOCALLY_HOMED_ADDRESS",
        "Experimental": "1",
        "PerPkg": "1",
        "PublicDescription": "Cache Lookups : Transactions homed locally",
        "UMask": "0xbdfff",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "Cache Lookups: Code Read Requests and Code Read Prefetches to Locally Homed Memory",
        "Counter": "0,1,2,3",
        "EventCode": "0x34",
        "EventName": "UNC_CHA_LLC_LOOKUP.LOCAL_CODE",
        "Experimental": "1",
        "PerPkg": "1",
        "PublicDescription": "Cache Lookups : CRd Requests",
        "UMask": "0x19d0ff",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "Cache Lookups: Read Requests and Read Prefetches to Locally Homed Memory",
        "Counter": "0,1,2,3",
        "EventCode": "0x34",
        "EventName": "UNC_CHA_LLC_LOOKUP.LOCAL_DATA_RD",
        "Experimental": "1",
        "PerPkg": "1",
        "PublicDescription": "Counts the number of times the LLC was accessed - this includes code, data, prefetches and hints coming from L2.  This has numerous filters available.  Note the non-standard filtering equation.  This event will count requests that lookup the cache multiple times with multiple increments.  One must ALWAYS set umask bit 0 and select a state or states to match.  Otherwise, the event will count nothing.   CHAFilter0[24:21,17] bits correspond to [FMESI] state. Read transactions",
        "UMask": "0x19c1ff",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "Cache Lookups: Code Read Requests to Locally Homed Memory",
        "Counter": "0,1,2,3",
        "EventCode": "0x34",
        "EventName": "UNC_CHA_LLC_LOOKUP.LOCAL_DMND_CODE",
        "Experimental": "1",
        "PerPkg": "1",
        "PublicDescription": "Cache Lookups : CRd Requests",
        "UMask": "0x1850ff",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "Cache Lookups: Read Requests to Locally Homed Memory",
        "Counter": "0,1,2,3",
        "EventCode": "0x34",
        "EventName": "UNC_CHA_LLC_LOOKUP.LOCAL_DMND_DATA_RD",
        "Experimental": "1",
        "PerPkg": "1",
        "PublicDescription": "Counts the number of times the LLC was accessed - this includes code, data, prefetches and hints coming from L2.  This has numerous filters available.  Note the non-standard filtering equation.  This event will count requests that lookup the cache multiple times with multiple increments.  One must ALWAYS set umask bit 0 and select a state or states to match.  Otherwise, the event will count nothing.   CHAFilter0[24:21,17] bits correspond to [FMESI] state. Read transactions",
        "UMask": "0x1841ff",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "Cache Lookups: RFO Requests to Locally Homed Memory",
        "Counter": "0,1,2,3",
        "EventCode": "0x34",
        "EventName": "UNC_CHA_LLC_LOOKUP.LOCAL_DMND_RFO",
        "Experimental": "1",
        "PerPkg": "1",
        "PublicDescription": "Cache Lookups : RFO Requests",
        "UMask": "0x1848ff",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "Cache Lookups: LLC Prefetch Requests to Locally Homed Memory",
        "Counter": "0,1,2,3",
        "EventCode": "0x34",
        "EventName": "UNC_CHA_LLC_LOOKUP.LOCAL_LLC_PF",
        "Experimental": "1",
        "PerPkg": "1",
        "PublicDescription": "Counts the number of times the LLC was accessed - this includes code, data, prefetches and hints coming from L2.  This has numerous filters available.  Note the non-standard filtering equation.  This event will count requests that lookup the cache multiple times with multiple increments.  One must ALWAYS set umask bit 0 and select a state or states to match.  Otherwise, the event will count nothing.   CHAFilter0[24:21,17] bits correspond to [FMESI] state. Read transactions",
        "UMask": "0x189dff",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "Cache Lookups: All Prefetches to Locally Homed Memory",
        "Counter": "0,1,2,3",
        "EventCode": "0x34",
        "EventName": "UNC_CHA_LLC_LOOKUP.LOCAL_PF",
        "Experimental": "1",
        "PerPkg": "1",
        "PublicDescription": "Counts the number of times the LLC was accessed - this includes code, data, prefetches and hints coming from L2.  This has numerous filters available.  Note the non-standard filtering equation.  This event will count requests that lookup the cache multiple times with multiple increments.  One must ALWAYS set umask bit 0 and select a state or states to match.  Otherwise, the event will count nothing.   CHAFilter0[24:21,17] bits correspond to [FMESI] state. Read transactions",
        "UMask": "0x199dff",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "Cache Lookups: Code Prefetches to Locally Homed Memory",
        "Counter": "0,1,2,3",
        "EventCode": "0x34",
        "EventName": "UNC_CHA_LLC_LOOKUP.LOCAL_PF_CODE",
        "Experimental": "1",
        "PerPkg": "1",
        "PublicDescription": "Cache Lookups : CRd Requests",
        "UMask": "0x1910ff",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "Cache Lookups: Read Prefetches to Locally Homed Memory",
        "Counter": "0,1,2,3",
        "EventCode": "0x34",
        "EventName": "UNC_CHA_LLC_LOOKUP.LOCAL_PF_DATA_RD",
        "Experimental": "1",
        "PerPkg": "1",
        "PublicDescription": "Counts the number of times the LLC was accessed - this includes code, data, prefetches and hints coming from L2.  This has numerous filters available.  Note the non-standard filtering equation.  This event will count requests that lookup the cache multiple times with multiple increments.  One must ALWAYS set umask bit 0 and select a state or states to match.  Otherwise, the event will count nothing.   CHAFilter0[24:21,17] bits correspond to [FMESI] state. Read transactions",
        "UMask": "0x1981ff",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "Cache Lookups: RFO Prefetches to Locally Homed Memory",
        "Counter": "0,1,2,3",
        "EventCode": "0x34",
        "EventName": "UNC_CHA_LLC_LOOKUP.LOCAL_PF_RFO",
        "Experimental": "1",
        "PerPkg": "1",
        "PublicDescription": "Cache Lookups : RFO Requests",
        "UMask": "0x1908ff",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "Cache Lookups: RFO Requests and RFO Prefetches to Locally Homed Memory",
        "Counter": "0,1,2,3",
        "EventCode": "0x34",
        "EventName": "UNC_CHA_LLC_LOOKUP.LOCAL_RFO",
        "Experimental": "1",
        "PerPkg": "1",
        "PublicDescription": "Cache Lookups : RFO Requests",
        "UMask": "0x19c8ff",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "Cache Lookups: All RFO and RFO Prefetches",
        "Counter": "0,1,2,3",
        "EventCode": "0x34",
        "EventName": "UNC_CHA_LLC_LOOKUP.RFO",
        "Experimental": "1",
        "PerPkg": "1",
        "PublicDescription": "Cache Lookups : All RFOs - Demand and Prefetches",
        "UMask": "0x1bc8ff",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "Cache Lookups: RFO Requests and RFO Prefetches to Locally Homed Memory",
        "Counter": "0,1,2,3",
        "EventCode": "0x34",
        "EventName": "UNC_CHA_LLC_LOOKUP.RFO_LOCAL",
        "Experimental": "1",
        "PerPkg": "1",
        "PublicDescription": "Cache Lookups : Locally HOMed RFOs - Demand and Prefetches",
        "UMask": "0x9c8ff",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "Cache Lookups: Writes to Locally Homed Memory (includes writebacks from L1/L2)",
        "Counter": "0,1,2,3",
        "EventCode": "0x34",
        "EventName": "UNC_CHA_LLC_LOOKUP.WRITE_LOCAL",
        "Experimental": "1",
        "PerPkg": "1",
        "PublicDescription": "Cache Lookups : Writes",
        "UMask": "0x842ff",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "Counts the number of lines that were victimized on a fill.  This can be filtered by the state that the line was in.",
        "Counter": "0,1,2,3",
        "EventCode": "0x37",
        "EventName": "UNC_CHA_LLC_VICTIMS.ALL",
        "Experimental": "1",
        "PerPkg": "1",
        "PublicDescription": "Lines Victimized : All Lines Victimized",
        "UMask": "0xf",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "Lines Victimized : IA traffic : Counts the number of lines that were victimized on a fill.  This can be filtered by the state that the line was in.",
        "Counter": "0,1,2,3",
        "EventCode": "0x37",
        "EventName": "UNC_CHA_LLC_VICTIMS.IA",
        "Experimental": "1",
        "PerPkg": "1",
        "UMask": "0x20",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "Lines Victimized : IO traffic : Counts the number of lines that were victimized on a fill.  This can be filtered by the state that the line was in.",
        "Counter": "0,1,2,3",
        "EventCode": "0x37",
        "EventName": "UNC_CHA_LLC_VICTIMS.IO",
        "Experimental": "1",
        "PerPkg": "1",
        "UMask": "0x10",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "Counts the number of lines that were victimized on a fill.  This can be filtered by the state that the line was in.",
        "Counter": "0,1,2,3",
        "EventCode": "0x37",
        "EventName": "UNC_CHA_LLC_VICTIMS.LOCAL_ALL",
        "Experimental": "1",
        "PerPkg": "1",
        "PublicDescription": "Lines Victimized : Local - All Lines",
        "UMask": "0x200f",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "Lines Victimized : Counts the number of lines that were victimized on a fill.  This can be filtered by the state that the line was in.",
        "Counter": "0,1,2,3",
        "EventCode": "0x37",
        "EventName": "UNC_CHA_LLC_VICTIMS.LOCAL_E",
        "Experimental": "1",
        "PerPkg": "1",
        "PublicDescription": "Lines Victimized : Local - Lines in E State",
        "UMask": "0x2002",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "Lines Victimized : Counts the number of lines that were victimized on a fill.  This can be filtered by the state that the line was in.",
        "Counter": "0,1,2,3",
        "EventCode": "0x37",
        "EventName": "UNC_CHA_LLC_VICTIMS.LOCAL_F",
        "Experimental": "1",
        "PerPkg": "1",
        "PublicDescription": "Lines Victimized : Local - Lines in F State",
        "UMask": "0x2008",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "Lines Victimized : Counts the number of lines that were victimized on a fill.  This can be filtered by the state that the line was in.",
        "Counter": "0,1,2,3",
        "EventCode": "0x37",
        "EventName": "UNC_CHA_LLC_VICTIMS.LOCAL_M",
        "Experimental": "1",
        "PerPkg": "1",
        "PublicDescription": "Lines Victimized : Local - Lines in M State",
        "UMask": "0x2001",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "Lines Victimized : Counts the number of lines that were victimized on a fill.  This can be filtered by the state that the line was in.",
        "Counter": "0,1,2,3",
        "EventCode": "0x37",
        "EventName": "UNC_CHA_LLC_VICTIMS.LOCAL_S",
        "Experimental": "1",
        "PerPkg": "1",
        "PublicDescription": "Lines Victimized : Local - Lines in S State",
        "UMask": "0x2004",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "Counts the number of lines that were victimized on a fill.  This can be filtered by the state that the line was in.",
        "Counter": "0,1,2,3",
        "EventCode": "0x37",
        "EventName": "UNC_CHA_LLC_VICTIMS.TOTAL_E",
        "Experimental": "1",
        "PerPkg": "1",
        "PublicDescription": "Lines Victimized : Lines in E state",
        "UMask": "0x2",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "Counts the number of lines that were victimized on a fill.  This can be filtered by the state that the line was in.",
        "Counter": "0,1,2,3",
        "EventCode": "0x37",
        "EventName": "UNC_CHA_LLC_VICTIMS.TOTAL_M",
        "Experimental": "1",
        "PerPkg": "1",
        "PublicDescription": "Lines Victimized : Lines in M state",
        "UMask": "0x1",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "Counts the number of lines that were victimized on a fill.  This can be filtered by the state that the line was in.",
        "Counter": "0,1,2,3",
        "EventCode": "0x37",
        "EventName": "UNC_CHA_LLC_VICTIMS.TOTAL_S",
        "Experimental": "1",
        "PerPkg": "1",
        "PublicDescription": "Lines Victimized : Lines in S State",
        "UMask": "0x4",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "Counts when a RFO (the Read for Ownership issued before a  write) request hit a cacheline in the S (Shared) state.",
        "Counter": "0,1,2,3",
        "EventCode": "0x39",
        "EventName": "UNC_CHA_MISC.RFO_HIT_S",
        "PerPkg": "1",
        "PublicDescription": "Cbo Misc : RFO HitS",
        "UMask": "0x8",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "OSB Snoop Broadcast : Local InvItoE : Count of OSB snoop broadcasts. Counts by 1 per request causing OSB snoops to be broadcast. Does not count all the snoops generated by OSB.",
        "Counter": "0,1,2,3",
        "EventCode": "0x55",
        "EventName": "UNC_CHA_OSB.LOCAL_INVITOE",
        "Experimental": "1",
        "PerPkg": "1",
        "UMask": "0x1",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "OSB Snoop Broadcast : Local Rd : Count of OSB snoop broadcasts. Counts by 1 per request causing OSB snoops to be broadcast. Does not count all the snoops generated by OSB.",
        "Counter": "0,1,2,3",
        "EventCode": "0x55",
        "EventName": "UNC_CHA_OSB.LOCAL_READ",
        "Experimental": "1",
        "PerPkg": "1",
        "UMask": "0x2",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "OSB Snoop Broadcast : Off : Count of OSB snoop broadcasts. Counts by 1 per request causing OSB snoops to be broadcast. Does not count all the snoops generated by OSB.",
        "Counter": "0,1,2,3",
        "EventCode": "0x55",
        "EventName": "UNC_CHA_OSB.OFF_PWRHEURISTIC",
        "Experimental": "1",
        "PerPkg": "1",
        "UMask": "0x20",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "OSB Snoop Broadcast : RFO HitS Snoop Broadcast : Count of OSB snoop broadcasts. Counts by 1 per request causing OSB snoops to be broadcast. Does not count all the snoops generated by OSB.",
        "Counter": "0,1,2,3",
        "EventCode": "0x55",
        "EventName": "UNC_CHA_OSB.RFO_HITS_SNP_BCAST",
        "PerPkg": "1",
        "UMask": "0x10",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "Counts the total number of requests coming from a unit on this socket for exclusive ownership of a cache line without receiving data (INVITOE) to the CHA.",
        "Counter": "0,1,2,3",
        "EventCode": "0x50",
        "EventName": "UNC_CHA_REQUESTS.INVITOE",
        "PerPkg": "1",
        "PublicDescription": "HA Read and Write Requests : InvalItoE",
        "UMask": "0x30",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "Counts the total number of requests coming from a unit on this socket for exclusive ownership of a cache line without receiving data (INVITOE) to the CHA.",
        "Counter": "0,1,2,3",
        "EventCode": "0x50",
        "EventName": "UNC_CHA_REQUESTS.INVITOE_LOCAL",
        "PerPkg": "1",
        "UMask": "0x10",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "Counts read requests made into this CHA. Reads include all read opcodes (including RFO: the Read for Ownership issued before a  write) .",
        "Counter": "0,1,2,3",
        "EventCode": "0x50",
        "EventName": "UNC_CHA_REQUESTS.READS",
        "PerPkg": "1",
        "PublicDescription": "HA Read and Write Requests : Reads",
        "UMask": "0x3",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "Counts read requests coming from a unit on this socket made into this CHA. Reads include all read opcodes (including RFO: the Read for Ownership issued before a  write).",
        "Counter": "0,1,2,3",
        "EventCode": "0x50",
        "EventName": "UNC_CHA_REQUESTS.READS_LOCAL",
        "PerPkg": "1",
        "UMask": "0x1",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "Counts write requests made into the CHA, including streaming, evictions, HitM (Reads from another core to a Modified cacheline), etc.",
        "Counter": "0,1,2,3",
        "EventCode": "0x50",
        "EventName": "UNC_CHA_REQUESTS.WRITES",
        "PerPkg": "1",
        "PublicDescription": "HA Read and Write Requests : Writes",
        "UMask": "0xc",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "Counts  write requests coming from a unit on this socket made into this CHA, including streaming, evictions, HitM (Reads from another core to a Modified cacheline), etc.",
        "Counter": "0,1,2,3",
        "EventCode": "0x50",
        "EventName": "UNC_CHA_REQUESTS.WRITES_LOCAL",
        "PerPkg": "1",
        "UMask": "0x4",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "Ingress (from CMS) Allocations : IRQ : Counts number of allocations per cycle into the specified Ingress queue.",
        "Counter": "0,1,2,3",
        "EventCode": "0x13",
        "EventName": "UNC_CHA_RxC_INSERTS.IRQ",
        "Experimental": "1",
        "PerPkg": "1",
        "UMask": "0x1",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "Ingress (from CMS) Occupancy : IRQ : Counts number of entries in the specified Ingress queue in each cycle.",
        "Counter": "0",
        "EventCode": "0x11",
        "EventName": "UNC_CHA_RxC_OCCUPANCY.IRQ",
        "Experimental": "1",
        "PerPkg": "1",
        "UMask": "0x1",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "All TOR Inserts",
        "Counter": "0,1,2,3",
        "EventCode": "0x35",
        "EventName": "UNC_CHA_TOR_INSERTS.ALL",
        "Experimental": "1",
        "PerPkg": "1",
        "PublicDescription": "TOR Inserts : All",
        "UMask": "0xc001ffff",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "All locally initiated requests from IA Cores",
        "Counter": "0,1,2,3",
        "EventCode": "0x35",
        "EventName": "UNC_CHA_TOR_INSERTS.IA",
        "Experimental": "1",
        "PerPkg": "1",
        "PublicDescription": "TOR Inserts : All requests from iA Cores",
        "UMask": "0xc001ff01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "CLFlush events that are initiated from the Core",
        "Counter": "0,1,2,3",
        "EventCode": "0x35",
        "EventName": "UNC_CHA_TOR_INSERTS.IA_CLFLUSH",
        "PerPkg": "1",
        "PublicDescription": "TOR Inserts : CLFlushes issued by iA Cores",
        "UMask": "0xc8c7ff01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "CLFlushOpt events that are initiated from the Core",
        "Counter": "0,1,2,3",
        "EventCode": "0x35",
        "EventName": "UNC_CHA_TOR_INSERTS.IA_CLFLUSHOPT",
        "PerPkg": "1",
        "PublicDescription": "TOR Inserts : CLFlushOpts issued by iA Cores",
        "UMask": "0xc8d7ff01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "Code read from local IA",
        "Counter": "0,1,2,3",
        "EventCode": "0x35",
        "EventName": "UNC_CHA_TOR_INSERTS.IA_CRD",
        "PerPkg": "1",
        "PublicDescription": "TOR Inserts : CRDs issued by iA Cores",
        "UMask": "0xc80fff01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "Code read prefetch from local IA that miss the cache",
        "Counter": "0,1,2,3",
        "EventCode": "0x35",
        "EventName": "UNC_CHA_TOR_INSERTS.IA_CRD_PREF",
        "PerPkg": "1",
        "PublicDescription": "TOR Inserts; Code read prefetch from local IA that misses in the snoop filter",
        "UMask": "0xc88fff01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "Data read opt from local IA",
        "Counter": "0,1,2,3",
        "EventCode": "0x35",
        "EventName": "UNC_CHA_TOR_INSERTS.IA_DRD_OPT",
        "PerPkg": "1",
        "PublicDescription": "TOR Inserts : DRd_Opts issued by iA Cores",
        "UMask": "0xc827ff01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "Data read opt prefetch from local IA",
        "Counter": "0,1,2,3",
        "EventCode": "0x35",
        "EventName": "UNC_CHA_TOR_INSERTS.IA_DRD_OPT_PREF",
        "PerPkg": "1",
        "PublicDescription": "TOR Inserts : DRd_Opt_Prefs issued by iA Cores",
        "UMask": "0xc8a7ff01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "All locally initiated requests from IA Cores which hit the cache",
        "Counter": "0,1,2,3",
        "EventCode": "0x35",
        "EventName": "UNC_CHA_TOR_INSERTS.IA_HIT",
        "Experimental": "1",
        "PerPkg": "1",
        "PublicDescription": "TOR Inserts : All requests from iA Cores that Hit the LLC",
        "UMask": "0xc001fd01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "Code read from local IA that hit the cache",
        "Counter": "0,1,2,3",
        "EventCode": "0x35",
        "EventName": "UNC_CHA_TOR_INSERTS.IA_HIT_CRD",
        "PerPkg": "1",
        "PublicDescription": "TOR Inserts : CRds issued by iA Cores that Hit the LLC",
        "UMask": "0xc80ffd01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "Code read prefetch from local IA that hit the cache",
        "Counter": "0,1,2,3",
        "EventCode": "0x35",
        "EventName": "UNC_CHA_TOR_INSERTS.IA_HIT_CRD_PREF",
        "PerPkg": "1",
        "PublicDescription": "TOR Inserts : CRd_Prefs issued by iA Cores that hit the LLC",
        "UMask": "0xc88ffd01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "Data read opt from local IA that hit the cache",
        "Counter": "0,1,2,3",
        "EventCode": "0x35",
        "EventName": "UNC_CHA_TOR_INSERTS.IA_HIT_DRD_OPT",
        "PerPkg": "1",
        "PublicDescription": "TOR Inserts : DRd_Opts issued by iA Cores that hit the LLC",
        "UMask": "0xc827fd01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "Data read opt prefetch from local IA that hit the cache",
        "Counter": "0,1,2,3",
        "EventCode": "0x35",
        "EventName": "UNC_CHA_TOR_INSERTS.IA_HIT_DRD_OPT_PREF",
        "PerPkg": "1",
        "PublicDescription": "TOR Inserts : DRd_Opt_Prefs issued by iA Cores that hit the LLC",
        "UMask": "0xc8a7fd01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "ItoM requests from local IA cores that hit the cache",
        "Counter": "0,1,2,3",
        "EventCode": "0x35",
        "EventName": "UNC_CHA_TOR_INSERTS.IA_HIT_ITOM",
        "PerPkg": "1",
        "PublicDescription": "TOR Inserts : ItoMs issued by iA Cores that Hit LLC",
        "UMask": "0xcc47fd01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "Last level cache prefetch code read from local IA that hit the cache",
        "Counter": "0,1,2,3",
        "EventCode": "0x35",
        "EventName": "UNC_CHA_TOR_INSERTS.IA_HIT_LLCPREFCODE",
        "PerPkg": "1",
        "PublicDescription": "TOR Inserts : LLCPrefCode issued by iA Cores that hit the LLC",
        "UMask": "0xcccffd01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "Last level cache prefetch data read from local IA that hit the cache",
        "Counter": "0,1,2,3",
        "EventCode": "0x35",
        "EventName": "UNC_CHA_TOR_INSERTS.IA_HIT_LLCPREFDATA",
        "PerPkg": "1",
        "PublicDescription": "TOR Inserts : LLCPrefData issued by iA Cores that hit the LLC",
        "UMask": "0xccd7fd01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "Last level cache prefetch read for ownership from local IA that hit the cache",
        "Counter": "0,1,2,3",
        "EventCode": "0x35",
        "EventName": "UNC_CHA_TOR_INSERTS.IA_HIT_LLCPREFRFO",
        "PerPkg": "1",
        "PublicDescription": "TOR Inserts : LLCPrefRFO issued by iA Cores that hit the LLC",
        "UMask": "0xccc7fd01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "Read for ownership from local IA that hit the cache",
        "Counter": "0,1,2,3",
        "EventCode": "0x35",
        "EventName": "UNC_CHA_TOR_INSERTS.IA_HIT_RFO",
        "PerPkg": "1",
        "PublicDescription": "TOR Inserts : RFOs issued by iA Cores that Hit the LLC",
        "UMask": "0xc807fd01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "Read for ownership prefetch from local IA that hit the cache",
        "Counter": "0,1,2,3",
        "EventCode": "0x35",
        "EventName": "UNC_CHA_TOR_INSERTS.IA_HIT_RFO_PREF",
        "PerPkg": "1",
        "PublicDescription": "TOR Inserts : RFO_Prefs issued by iA Cores that Hit the LLC",
        "UMask": "0xc887fd01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "ItoM events that are initiated from the Core",
        "Counter": "0,1,2,3",
        "EventCode": "0x35",
        "EventName": "UNC_CHA_TOR_INSERTS.IA_ITOM",
        "PerPkg": "1",
        "PublicDescription": "TOR Inserts : ItoMs issued by iA Cores",
        "UMask": "0xcc47ff01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "ItoMCacheNear requests from local IA cores",
        "Counter": "0,1,2,3",
        "EventCode": "0x35",
        "EventName": "UNC_CHA_TOR_INSERTS.IA_ITOMCACHENEAR",
        "PerPkg": "1",
        "PublicDescription": "TOR Inserts : ItoMCacheNears issued by iA Cores",
        "UMask": "0xcd47ff01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "Last level cache prefetch code read from local IA.",
        "Counter": "0,1,2,3",
        "EventCode": "0x35",
        "EventName": "UNC_CHA_TOR_INSERTS.IA_LLCPREFCODE",
        "PerPkg": "1",
        "PublicDescription": "TOR Inserts : LLCPrefCode issued by iA Cores",
        "UMask": "0xcccfff01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "Last level cache prefetch data read from local IA.",
        "Counter": "0,1,2,3",
        "EventCode": "0x35",
        "EventName": "UNC_CHA_TOR_INSERTS.IA_LLCPREFDATA",
        "PerPkg": "1",
        "PublicDescription": "TOR Inserts : LLCPrefData issued by iA Cores",
        "UMask": "0xccd7ff01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "Last level cache prefetch read for ownership from local IA",
        "Counter": "0,1,2,3",
        "EventCode": "0x35",
        "EventName": "UNC_CHA_TOR_INSERTS.IA_LLCPREFRFO",
        "PerPkg": "1",
        "PublicDescription": "TOR Inserts : LLCPrefRFO issued by iA Cores",
        "UMask": "0xccc7ff01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "All locally initiated requests from IA Cores which miss the cache",
        "Counter": "0,1,2,3",
        "EventCode": "0x35",
        "EventName": "UNC_CHA_TOR_INSERTS.IA_MISS",
        "PerPkg": "1",
        "PublicDescription": "TOR Inserts : All requests from iA Cores that Missed the LLC",
        "UMask": "0xc001fe01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "Code read from local IA that miss the cache",
        "Counter": "0,1,2,3",
        "EventCode": "0x35",
        "EventName": "UNC_CHA_TOR_INSERTS.IA_MISS_CRD",
        "PerPkg": "1",
        "PublicDescription": "TOR Inserts : CRds issued by iA Cores that Missed the LLC",
        "UMask": "0xc80ffe01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "CRDs from local IA cores to locally homed memory",
        "Counter": "0,1,2,3",
        "EventCode": "0x35",
        "EventName": "UNC_CHA_TOR_INSERTS.IA_MISS_CRD_LOCAL",
        "PerPkg": "1",
        "PublicDescription": "TOR Inserts : CRd issued by iA Cores that Missed the LLC - HOMed locally",
        "UMask": "0xc80efe01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "Code read prefetch from local IA that miss the cache",
        "Counter": "0,1,2,3",
        "EventCode": "0x35",
        "EventName": "UNC_CHA_TOR_INSERTS.IA_MISS_CRD_PREF",
        "PerPkg": "1",
        "PublicDescription": "TOR Inserts : CRd_Prefs issued by iA Cores that Missed the LLC",
        "UMask": "0xc88ffe01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "CRD Prefetches from local IA cores to locally homed memory",
        "Counter": "0,1,2,3",
        "EventCode": "0x35",
        "EventName": "UNC_CHA_TOR_INSERTS.IA_MISS_CRD_PREF_LOCAL",
        "PerPkg": "1",
        "PublicDescription": "TOR Inserts : CRd_Prefs issued by iA Cores that Missed the LLC - HOMed locally",
        "UMask": "0xc88efe01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "Data read opt from local IA that miss the cache",
        "Counter": "0,1,2,3",
        "EventCode": "0x35",
        "EventName": "UNC_CHA_TOR_INSERTS.IA_MISS_DRD_OPT",
        "PerPkg": "1",
        "PublicDescription": "TOR Inserts : DRd_Opt issued by iA Cores that missed the LLC",
        "UMask": "0xc827fe01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "Inserts into the TOR from local IA cores which miss the LLC and snoop filter with the opcode DRd_Opt, and which target local memory",
        "Counter": "0,1,2,3",
        "EventCode": "0x35",
        "EventName": "UNC_CHA_TOR_INSERTS.IA_MISS_DRD_OPT_LOCAL",
        "PerPkg": "1",
        "PublicDescription": "TOR Inserts : DRd_Opt issued by iA Cores that Missed the LLC - HOMed locally",
        "UMask": "0xc826fe01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "Data read opt prefetch from local IA that miss the cache",
        "Counter": "0,1,2,3",
        "EventCode": "0x35",
        "EventName": "UNC_CHA_TOR_INSERTS.IA_MISS_DRD_OPT_PREF",
        "PerPkg": "1",
        "PublicDescription": "TOR Inserts : DRd_Opt_Prefs issued by iA Cores that missed the LLC",
        "UMask": "0xc8a7fe01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "Inserts into the TOR from local IA cores which miss the LLC and snoop filter with the opcode DRD_PREF_OPT, and target local memory",
        "Counter": "0,1,2,3",
        "EventCode": "0x35",
        "EventName": "UNC_CHA_TOR_INSERTS.IA_MISS_DRD_OPT_PREF_LOCAL",
        "PerPkg": "1",
        "PublicDescription": "TOR Inserts : Data read opt prefetch from local iA that missed the LLC targeting local memory",
        "UMask": "0xc8a6fe01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "ItoM requests from local IA cores that miss the cache",
        "Counter": "0,1,2,3",
        "EventCode": "0x35",
        "EventName": "UNC_CHA_TOR_INSERTS.IA_MISS_ITOM",
        "PerPkg": "1",
        "PublicDescription": "TOR Inserts : ItoMs issued by iA Cores that Missed LLC",
        "UMask": "0xcc47fe01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "Last level cache prefetch code read from local IA that miss the cache",
        "Counter": "0,1,2,3",
        "EventCode": "0x35",
        "EventName": "UNC_CHA_TOR_INSERTS.IA_MISS_LLCPREFCODE",
        "PerPkg": "1",
        "PublicDescription": "TOR Inserts : LLCPrefCode issued by iA Cores that missed the LLC",
        "UMask": "0xcccffe01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "Last level cache prefetch data read from local IA that miss the cache",
        "Counter": "0,1,2,3",
        "EventCode": "0x35",
        "EventName": "UNC_CHA_TOR_INSERTS.IA_MISS_LLCPREFDATA",
        "PerPkg": "1",
        "PublicDescription": "TOR Inserts : LLCPrefData issued by iA Cores that missed the LLC",
        "UMask": "0xccd7fe01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "Last level cache prefetch read for ownership from local IA that miss the cache",
        "Counter": "0,1,2,3",
        "EventCode": "0x35",
        "EventName": "UNC_CHA_TOR_INSERTS.IA_MISS_LLCPREFRFO",
        "PerPkg": "1",
        "PublicDescription": "TOR Inserts : LLCPrefRFO issued by iA Cores that missed the LLC",
        "UMask": "0xccc7fe01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "WCILF requests from local IA cores to locally homed DDR addresses that miss the cache",
        "Counter": "0,1,2,3",
        "EventCode": "0x35",
        "EventName": "UNC_CHA_TOR_INSERTS.IA_MISS_LOCAL_WCILF_DDR",
        "PerPkg": "1",
        "PublicDescription": "TOR Inserts : WCiLFs issued by iA Cores targeting DDR that missed the LLC - HOMed locally",
        "UMask": "0xc8668601",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "WCIL requests from local IA cores to locally homed DDR addresses that miss the cache",
        "Counter": "0,1,2,3",
        "EventCode": "0x35",
        "EventName": "UNC_CHA_TOR_INSERTS.IA_MISS_LOCAL_WCIL_DDR",
        "PerPkg": "1",
        "PublicDescription": "TOR Inserts : WCiLs issued by iA Cores targeting DDR that missed the LLC - HOMed locally",
        "UMask": "0xc86e8601",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "Read for ownership from local IA that miss the cache",
        "Counter": "0,1,2,3",
        "EventCode": "0x35",
        "EventName": "UNC_CHA_TOR_INSERTS.IA_MISS_RFO",
        "PerPkg": "1",
        "PublicDescription": "TOR Inserts : RFOs issued by iA Cores that Missed the LLC",
        "UMask": "0xc807fe01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "Read for ownership from local IA that miss the LLC targeting local memory",
        "Counter": "0,1,2,3",
        "EventCode": "0x35",
        "EventName": "UNC_CHA_TOR_INSERTS.IA_MISS_RFO_LOCAL",
        "PerPkg": "1",
        "PublicDescription": "TOR Inserts : RFOs issued by iA Cores that Missed the LLC - HOMed locally",
        "UMask": "0xc806fe01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "Read for ownership prefetch from local IA that miss the cache",
        "Counter": "0,1,2,3",
        "EventCode": "0x35",
        "EventName": "UNC_CHA_TOR_INSERTS.IA_MISS_RFO_PREF",
        "PerPkg": "1",
        "PublicDescription": "TOR Inserts : RFO_Prefs issued by iA Cores that Missed the LLC",
        "UMask": "0xc887fe01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "Read for ownership prefetch from local IA that miss the LLC targeting local memory",
        "Counter": "0,1,2,3",
        "EventCode": "0x35",
        "EventName": "UNC_CHA_TOR_INSERTS.IA_MISS_RFO_PREF_LOCAL",
        "PerPkg": "1",
        "PublicDescription": "TOR Inserts : RFO_Prefs issued by iA Cores that Missed the LLC - HOMed locally",
        "UMask": "0xc886fe01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "UCRDF requests from local IA cores that miss the cache",
        "Counter": "0,1,2,3",
        "EventCode": "0x35",
        "EventName": "UNC_CHA_TOR_INSERTS.IA_MISS_UCRDF",
        "PerPkg": "1",
        "PublicDescription": "TOR Inserts : UCRdFs issued by iA Cores that Missed LLC",
        "UMask": "0xc877de01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "WCIL requests from a local IA core that miss the cache",
        "Counter": "0,1,2,3",
        "EventCode": "0x35",
        "EventName": "UNC_CHA_TOR_INSERTS.IA_MISS_WCIL",
        "PerPkg": "1",
        "PublicDescription": "TOR Inserts : WCiLs issued by iA Cores that Missed the LLC",
        "UMask": "0xc86ffe01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "WCILF requests from local IA core that miss the cache",
        "Counter": "0,1,2,3",
        "EventCode": "0x35",
        "EventName": "UNC_CHA_TOR_INSERTS.IA_MISS_WCILF",
        "PerPkg": "1",
        "PublicDescription": "TOR Inserts : WCiLF issued by iA Cores that Missed the LLC",
        "UMask": "0xc867fe01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "WCILF requests from local IA cores to DDR homed addresses which miss the cache",
        "Counter": "0,1,2,3",
        "EventCode": "0x35",
        "EventName": "UNC_CHA_TOR_INSERTS.IA_MISS_WCILF_DDR",
        "PerPkg": "1",
        "PublicDescription": "TOR Inserts : WCiLFs issued by iA Cores targeting DDR that missed the LLC",
        "UMask": "0xc8678601",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "WCIL requests from local IA cores to DDR homed addresses which miss the cache",
        "Counter": "0,1,2,3",
        "EventCode": "0x35",
        "EventName": "UNC_CHA_TOR_INSERTS.IA_MISS_WCIL_DDR",
        "PerPkg": "1",
        "PublicDescription": "TOR Inserts : WCiLs issued by iA Cores targeting DDR that missed the LLC",
        "UMask": "0xc86f8601",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "WIL requests from local IA cores that miss the cache",
        "Counter": "0,1,2,3",
        "EventCode": "0x35",
        "EventName": "UNC_CHA_TOR_INSERTS.IA_MISS_WIL",
        "PerPkg": "1",
        "PublicDescription": "TOR Inserts : WiLs issued by iA Cores that Missed LLC",
        "UMask": "0xc87fde01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "Read for ownership from local IA",
        "Counter": "0,1,2,3",
        "EventCode": "0x35",
        "EventName": "UNC_CHA_TOR_INSERTS.IA_RFO",
        "PerPkg": "1",
        "PublicDescription": "TOR Inserts : RFOs issued by iA Cores",
        "UMask": "0xc807ff01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "Read for ownership prefetch from local IA",
        "Counter": "0,1,2,3",
        "EventCode": "0x35",
        "EventName": "UNC_CHA_TOR_INSERTS.IA_RFO_PREF",
        "PerPkg": "1",
        "PublicDescription": "TOR Inserts : RFO_Prefs issued by iA Cores",
        "UMask": "0xc887ff01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "SpecItoM events that are initiated from the Core",
        "Counter": "0,1,2,3",
        "EventCode": "0x35",
        "EventName": "UNC_CHA_TOR_INSERTS.IA_SPECITOM",
        "PerPkg": "1",
        "PublicDescription": "TOR Inserts : SpecItoMs issued by iA Cores",
        "UMask": "0xcc57ff01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "WbEFtoEs issued by iA Cores.  (Non Modified Write Backs)",
        "Counter": "0,1,2,3",
        "EventCode": "0x35",
        "EventName": "UNC_CHA_TOR_INSERTS.IA_WBEFTOE",
        "PerPkg": "1",
        "PublicDescription": "TOR Inserts : ItoMs issued by IO Devices that Hit the LLC",
        "UMask": "0xcc3fff01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "WbEFtoIs issued by iA Cores .  (Non Modified Write Backs)",
        "Counter": "0,1,2,3",
        "EventCode": "0x35",
        "EventName": "UNC_CHA_TOR_INSERTS.IA_WBEFTOI",
        "PerPkg": "1",
        "PublicDescription": "TOR Inserts : ItoMs issued by IO Devices that Hit the LLC",
        "UMask": "0xcc37ff01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "WbMtoEs issued by iA Cores .  (Modified Write Backs)",
        "Counter": "0,1,2,3",
        "EventCode": "0x35",
        "EventName": "UNC_CHA_TOR_INSERTS.IA_WBMTOE",
        "PerPkg": "1",
        "PublicDescription": "TOR Inserts : ItoMs issued by IO Devices that Hit the LLC",
        "UMask": "0xcc2fff01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "WbMtoI requests from local IA cores",
        "Counter": "0,1,2,3",
        "EventCode": "0x35",
        "EventName": "UNC_CHA_TOR_INSERTS.IA_WBMTOI",
        "PerPkg": "1",
        "PublicDescription": "TOR Inserts : WbMtoIs issued by iA Cores",
        "UMask": "0xcc27ff01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "WbStoIs issued by iA Cores .  (Non Modified Write Backs)",
        "Counter": "0,1,2,3",
        "EventCode": "0x35",
        "EventName": "UNC_CHA_TOR_INSERTS.IA_WBSTOI",
        "PerPkg": "1",
        "PublicDescription": "TOR Inserts : ItoMs issued by IO Devices that Hit the LLC",
        "UMask": "0xcc67ff01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "WCIL requests from a local IA core",
        "Counter": "0,1,2,3",
        "EventCode": "0x35",
        "EventName": "UNC_CHA_TOR_INSERTS.IA_WCIL",
        "PerPkg": "1",
        "PublicDescription": "TOR Inserts : WCiLs issued by iA Cores",
        "UMask": "0xc86fff01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "WCILF requests from local IA core",
        "Counter": "0,1,2,3",
        "EventCode": "0x35",
        "EventName": "UNC_CHA_TOR_INSERTS.IA_WCILF",
        "PerPkg": "1",
        "PublicDescription": "TOR Inserts : WCiLF issued by iA Cores",
        "UMask": "0xc867ff01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "All TOR inserts from local IO devices",
        "Counter": "0,1,2,3",
        "EventCode": "0x35",
        "EventName": "UNC_CHA_TOR_INSERTS.IO",
        "Experimental": "1",
        "PerPkg": "1",
        "PublicDescription": "TOR Inserts : All requests from IO Devices",
        "UMask": "0xc001ff04",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "CLFlush requests from IO devices",
        "Counter": "0,1,2,3",
        "EventCode": "0x35",
        "EventName": "UNC_CHA_TOR_INSERTS.IO_CLFLUSH",
        "PerPkg": "1",
        "PublicDescription": "TOR Inserts : CLFlushes issued by IO Devices",
        "UMask": "0xc8c3ff04",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "All TOR inserts from local IO devices which hit the cache",
        "Counter": "0,1,2,3",
        "EventCode": "0x35",
        "EventName": "UNC_CHA_TOR_INSERTS.IO_HIT",
        "Experimental": "1",
        "PerPkg": "1",
        "PublicDescription": "TOR Inserts : All requests from IO Devices that hit the LLC",
        "UMask": "0xc001fd04",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "ItoMs from local IO devices which hit the cache",
        "Counter": "0,1,2,3",
        "EventCode": "0x35",
        "EventName": "UNC_CHA_TOR_INSERTS.IO_HIT_ITOM",
        "PerPkg": "1",
        "PublicDescription": "TOR Inserts : ItoMs issued by IO Devices that Hit the LLC",
        "UMask": "0xcc43fd04",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "ItoMCacheNears, indicating a partial write request, from IO Devices that hit the LLC",
        "Counter": "0,1,2,3",
        "EventCode": "0x35",
        "EventName": "UNC_CHA_TOR_INSERTS.IO_HIT_ITOMCACHENEAR",
        "PerPkg": "1",
        "PublicDescription": "TOR Inserts : ItoMCacheNears, indicating a partial write request, from IO Devices that hit the LLC",
        "UMask": "0xcd43fd04",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "PCIRDCURs issued by IO devices which hit the LLC",
        "Counter": "0,1,2,3",
        "EventCode": "0x35",
        "EventName": "UNC_CHA_TOR_INSERTS.IO_HIT_PCIRDCUR",
        "PerPkg": "1",
        "PublicDescription": "TOR Inserts : PCIRdCurs issued by IO Devices that hit the LLC",
        "UMask": "0xc8f3fd04",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "RFOs from local IO devices which hit the cache",
        "Counter": "0,1,2,3",
        "EventCode": "0x35",
        "EventName": "UNC_CHA_TOR_INSERTS.IO_HIT_RFO",
        "PerPkg": "1",
        "PublicDescription": "TOR Inserts : RFOs issued by IO Devices that hit the LLC",
        "UMask": "0xc803fd04",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "All TOR ItoM inserts from local IO devices",
        "Counter": "0,1,2,3",
        "EventCode": "0x35",
        "EventName": "UNC_CHA_TOR_INSERTS.IO_ITOM",
        "PerPkg": "1",
        "PublicDescription": "TOR Inserts : ItoMs issued by IO Devices",
        "UMask": "0xcc43ff04",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "ItoMCacheNears, indicating a partial write request, from IO Devices",
        "Counter": "0,1,2,3",
        "EventCode": "0x35",
        "EventName": "UNC_CHA_TOR_INSERTS.IO_ITOMCACHENEAR",
        "PerPkg": "1",
        "PublicDescription": "TOR Inserts : ItoMCacheNears, indicating a partial write request, from IO Devices",
        "UMask": "0xcd43ff04",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "All TOR inserts from local IO devices which miss the cache",
        "Counter": "0,1,2,3",
        "EventCode": "0x35",
        "EventName": "UNC_CHA_TOR_INSERTS.IO_MISS",
        "Experimental": "1",
        "PerPkg": "1",
        "PublicDescription": "TOR Inserts : All requests from IO Devices that missed the LLC",
        "UMask": "0xc001fe04",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "All TOR ItoM inserts from local IO devices which miss the cache",
        "Counter": "0,1,2,3",
        "EventCode": "0x35",
        "EventName": "UNC_CHA_TOR_INSERTS.IO_MISS_ITOM",
        "PerPkg": "1",
        "PublicDescription": "TOR Inserts : ItoMs issued by IO Devices that missed the LLC",
        "UMask": "0xcc43fe04",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "ItoMCacheNears, indicating a partial write request, from IO Devices that missed the LLC",
        "Counter": "0,1,2,3",
        "EventCode": "0x35",
        "EventName": "UNC_CHA_TOR_INSERTS.IO_MISS_ITOMCACHENEAR",
        "PerPkg": "1",
        "PublicDescription": "TOR Inserts : ItoMCacheNears, indicating a partial write request, from IO Devices that missed the LLC",
        "UMask": "0xcd43fe04",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "PCIRDCURs issued by IO devices which miss the LLC",
        "Counter": "0,1,2,3",
        "EventCode": "0x35",
        "EventName": "UNC_CHA_TOR_INSERTS.IO_MISS_PCIRDCUR",
        "PerPkg": "1",
        "PublicDescription": "TOR Inserts : PCIRdCurs issued by IO Devices that missed the LLC",
        "UMask": "0xc8f3fe04",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "All TOR RFO inserts from local IO devices which miss the cache",
        "Counter": "0,1,2,3",
        "EventCode": "0x35",
        "EventName": "UNC_CHA_TOR_INSERTS.IO_MISS_RFO",
        "PerPkg": "1",
        "PublicDescription": "TOR Inserts : RFOs issued by IO Devices that missed the LLC",
        "UMask": "0xc803fe04",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "PCIRDCURs issued by IO devices",
        "Counter": "0,1,2,3",
        "EventCode": "0x35",
        "EventName": "UNC_CHA_TOR_INSERTS.IO_PCIRDCUR",
        "PerPkg": "1",
        "PublicDescription": "TOR Inserts : PCIRdCurs issued by IO Devices",
        "UMask": "0xc8f3ff04",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "RFOs from local IO devices",
        "Counter": "0,1,2,3",
        "EventCode": "0x35",
        "EventName": "UNC_CHA_TOR_INSERTS.IO_RFO",
        "PerPkg": "1",
        "PublicDescription": "TOR Inserts : RFOs issued by IO Devices",
        "UMask": "0xc803ff04",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "WBMtoI requests from IO devices",
        "Counter": "0,1,2,3",
        "EventCode": "0x35",
        "EventName": "UNC_CHA_TOR_INSERTS.IO_WBMTOI",
        "PerPkg": "1",
        "PublicDescription": "TOR Inserts : WbMtoIs issued by IO Devices",
        "UMask": "0xcc23ff04",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "TOR Inserts for SF or LLC Evictions",
        "Counter": "0,1,2,3",
        "EventCode": "0x35",
        "EventName": "UNC_CHA_TOR_INSERTS.LLC_OR_SF_EVICTIONS",
        "PerPkg": "1",
        "PublicDescription": "TOR allocation occurred as a result of SF/LLC evictions (came from the ISMQ)",
        "UMask": "0xc001ff02",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "All locally initiated requests",
        "Counter": "0,1,2,3",
        "EventCode": "0x35",
        "EventName": "UNC_CHA_TOR_INSERTS.LOC_ALL",
        "Experimental": "1",
        "PerPkg": "1",
        "PublicDescription": "TOR Inserts : All from Local iA and IO",
        "UMask": "0xc000ff05",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "All from Local iA",
        "Counter": "0,1,2,3",
        "EventCode": "0x35",
        "EventName": "UNC_CHA_TOR_INSERTS.LOC_IA",
        "Experimental": "1",
        "PerPkg": "1",
        "PublicDescription": "TOR Inserts : All from Local iA",
        "UMask": "0xc000ff01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "All from Local IO",
        "Counter": "0,1,2,3",
        "EventCode": "0x35",
        "EventName": "UNC_CHA_TOR_INSERTS.LOC_IO",
        "Experimental": "1",
        "PerPkg": "1",
        "PublicDescription": "TOR Inserts : All from Local IO",
        "UMask": "0xc000ff04",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "Occupancy for all TOR entries",
        "Counter": "0",
        "EventCode": "0x36",
        "EventName": "UNC_CHA_TOR_OCCUPANCY.ALL",
        "Experimental": "1",
        "PerPkg": "1",
        "PublicDescription": "TOR Occupancy : All",
        "UMask": "0xc001ffff",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "TOR Occupancy for All locally initiated requests from IA Cores",
        "Counter": "0",
        "EventCode": "0x36",
        "EventName": "UNC_CHA_TOR_OCCUPANCY.IA",
        "Experimental": "1",
        "PerPkg": "1",
        "PublicDescription": "TOR Occupancy : All requests from iA Cores",
        "UMask": "0xc001ff01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "TOR Occupancy for CLFlush events that are initiated from the Core",
        "Counter": "0",
        "EventCode": "0x36",
        "EventName": "UNC_CHA_TOR_OCCUPANCY.IA_CLFLUSH",
        "PerPkg": "1",
        "PublicDescription": "TOR Occupancy : CLFlushes issued by iA Cores",
        "UMask": "0xc8c7ff01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "TOR Occupancy for CLFlushOpt events that are initiated from the Core",
        "Counter": "0",
        "EventCode": "0x36",
        "EventName": "UNC_CHA_TOR_OCCUPANCY.IA_CLFLUSHOPT",
        "PerPkg": "1",
        "PublicDescription": "TOR Occupancy : CLFlushOpts issued by iA Cores",
        "UMask": "0xc8d7ff01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "TOR Occupancy for Code read from local IA that miss the cache",
        "Counter": "0",
        "EventCode": "0x36",
        "EventName": "UNC_CHA_TOR_OCCUPANCY.IA_CRD",
        "PerPkg": "1",
        "PublicDescription": "TOR Occupancy : CRDs issued by iA Cores",
        "UMask": "0xc80fff01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "TOR Occupancy for Code read prefetch from local IA that miss the cache",
        "Counter": "0",
        "EventCode": "0x36",
        "EventName": "UNC_CHA_TOR_OCCUPANCY.IA_CRD_PREF",
        "PerPkg": "1",
        "PublicDescription": "TOR Occupancy; Code read prefetch from local IA that misses in the snoop filter",
        "UMask": "0xc88fff01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "TOR Occupancy for Data read opt from local IA that miss the cache",
        "Counter": "0",
        "EventCode": "0x36",
        "EventName": "UNC_CHA_TOR_OCCUPANCY.IA_DRD_OPT",
        "PerPkg": "1",
        "PublicDescription": "TOR Occupancy : DRd_Opts issued by iA Cores",
        "UMask": "0xc827ff01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "TOR Occupancy for Data read opt prefetch from local IA that miss the cache",
        "Counter": "0",
        "EventCode": "0x36",
        "EventName": "UNC_CHA_TOR_OCCUPANCY.IA_DRD_OPT_PREF",
        "Experimental": "1",
        "PerPkg": "1",
        "PublicDescription": "TOR Occupancy : DRd_Opt_Prefs issued by iA Cores",
        "UMask": "0xc8a7ff01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "TOR Occupancy for All locally initiated requests from IA Cores which hit the cache",
        "Counter": "0",
        "EventCode": "0x36",
        "EventName": "UNC_CHA_TOR_OCCUPANCY.IA_HIT",
        "Experimental": "1",
        "PerPkg": "1",
        "PublicDescription": "TOR Occupancy : All requests from iA Cores that Hit the LLC",
        "UMask": "0xc001fd01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "TOR Occupancy for Code read from local IA that hit the cache",
        "Counter": "0",
        "EventCode": "0x36",
        "EventName": "UNC_CHA_TOR_OCCUPANCY.IA_HIT_CRD",
        "PerPkg": "1",
        "PublicDescription": "TOR Occupancy : CRds issued by iA Cores that Hit the LLC",
        "UMask": "0xc80ffd01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "TOR Occupancy for Code read prefetch from local IA that hit the cache",
        "Counter": "0",
        "EventCode": "0x36",
        "EventName": "UNC_CHA_TOR_OCCUPANCY.IA_HIT_CRD_PREF",
        "PerPkg": "1",
        "PublicDescription": "TOR Occupancy : CRd_Prefs issued by iA Cores that hit the LLC",
        "UMask": "0xc88ffd01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "TOR Occupancy for Data read opt from local IA that hit the cache",
        "Counter": "0",
        "EventCode": "0x36",
        "EventName": "UNC_CHA_TOR_OCCUPANCY.IA_HIT_DRD_OPT",
        "Experimental": "1",
        "PerPkg": "1",
        "PublicDescription": "TOR Occupancy : DRd_Opts issued by iA Cores that hit the LLC",
        "UMask": "0xc827fd01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "TOR Occupancy for Data read opt prefetch from local IA that hit the cache",
        "Counter": "0",
        "EventCode": "0x36",
        "EventName": "UNC_CHA_TOR_OCCUPANCY.IA_HIT_DRD_OPT_PREF",
        "Experimental": "1",
        "PerPkg": "1",
        "PublicDescription": "TOR Occupancy : DRd_Opt_Prefs issued by iA Cores that hit the LLC",
        "UMask": "0xc8a7fd01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "TOR Occupancy for ItoM requests from local IA cores that hit the cache",
        "Counter": "0",
        "EventCode": "0x36",
        "EventName": "UNC_CHA_TOR_OCCUPANCY.IA_HIT_ITOM",
        "PerPkg": "1",
        "PublicDescription": "TOR Occupancy : ItoMs issued by iA Cores that Hit LLC",
        "UMask": "0xcc47fd01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "TOR Occupancy for Last level cache prefetch code read from local IA that hit the cache",
        "Counter": "0",
        "EventCode": "0x36",
        "EventName": "UNC_CHA_TOR_OCCUPANCY.IA_HIT_LLCPREFCODE",
        "PerPkg": "1",
        "PublicDescription": "TOR Occupancy : LLCPrefCode issued by iA Cores that hit the LLC",
        "UMask": "0xcccffd01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "TOR Occupancy for Last level cache prefetch data read from local IA that hit the cache",
        "Counter": "0",
        "EventCode": "0x36",
        "EventName": "UNC_CHA_TOR_OCCUPANCY.IA_HIT_LLCPREFDATA",
        "PerPkg": "1",
        "PublicDescription": "TOR Occupancy : LLCPrefData issued by iA Cores that hit the LLC",
        "UMask": "0xccd7fd01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "TOR Occupancy for Last level cache prefetch read for ownership from local IA that hit the cache",
        "Counter": "0",
        "EventCode": "0x36",
        "EventName": "UNC_CHA_TOR_OCCUPANCY.IA_HIT_LLCPREFRFO",
        "PerPkg": "1",
        "PublicDescription": "TOR Occupancy : LLCPrefRFO issued by iA Cores that hit the LLC",
        "UMask": "0xccc7fd01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "TOR Occupancy for Read for ownership from local IA that hit the cache",
        "Counter": "0",
        "EventCode": "0x36",
        "EventName": "UNC_CHA_TOR_OCCUPANCY.IA_HIT_RFO",
        "PerPkg": "1",
        "PublicDescription": "TOR Occupancy : RFOs issued by iA Cores that Hit the LLC",
        "UMask": "0xc807fd01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "TOR Occupancy for Read for ownership prefetch from local IA that hit the cache",
        "Counter": "0",
        "EventCode": "0x36",
        "EventName": "UNC_CHA_TOR_OCCUPANCY.IA_HIT_RFO_PREF",
        "PerPkg": "1",
        "PublicDescription": "TOR Occupancy : RFO_Prefs issued by iA Cores that Hit the LLC",
        "UMask": "0xc887fd01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "TOR Occupancy for ItoM events that are initiated from the Core",
        "Counter": "0",
        "EventCode": "0x36",
        "EventName": "UNC_CHA_TOR_OCCUPANCY.IA_ITOM",
        "PerPkg": "1",
        "PublicDescription": "TOR Occupancy : ItoMs issued by iA Cores",
        "UMask": "0xcc47ff01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "TOR Occupancy for ItoMCacheNear requests from local IA cores",
        "Counter": "0",
        "EventCode": "0x36",
        "EventName": "UNC_CHA_TOR_OCCUPANCY.IA_ITOMCACHENEAR",
        "PerPkg": "1",
        "PublicDescription": "TOR Occupancy : ItoMCacheNears issued by iA Cores",
        "UMask": "0xcd47ff01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "TOR Occupancy for Last level cache prefetch code read from local IA.",
        "Counter": "0",
        "EventCode": "0x36",
        "EventName": "UNC_CHA_TOR_OCCUPANCY.IA_LLCPREFCODE",
        "PerPkg": "1",
        "PublicDescription": "TOR Occupancy : LLCPrefCode issued by iA Cores",
        "UMask": "0xcccfff01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "TOR Occupancy for Last level cache prefetch data read from local IA.",
        "Counter": "0",
        "EventCode": "0x36",
        "EventName": "UNC_CHA_TOR_OCCUPANCY.IA_LLCPREFDATA",
        "PerPkg": "1",
        "PublicDescription": "TOR Occupancy : LLCPrefData issued by iA Cores",
        "UMask": "0xccd7ff01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "TOR Occupancy for Last level cache prefetch read for ownership from local IA that miss the cache",
        "Counter": "0",
        "EventCode": "0x36",
        "EventName": "UNC_CHA_TOR_OCCUPANCY.IA_LLCPREFRFO",
        "PerPkg": "1",
        "PublicDescription": "TOR Occupancy : LLCPrefRFO issued by iA Cores",
        "UMask": "0xccc7ff01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "TOR Occupancy for All locally initiated requests from IA Cores which miss the cache",
        "Counter": "0",
        "EventCode": "0x36",
        "EventName": "UNC_CHA_TOR_OCCUPANCY.IA_MISS",
        "Experimental": "1",
        "PerPkg": "1",
        "PublicDescription": "TOR Occupancy : All requests from iA Cores that Missed the LLC",
        "UMask": "0xc001fe01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "TOR Occupancy for Code read from local IA that miss the cache",
        "Counter": "0",
        "EventCode": "0x36",
        "EventName": "UNC_CHA_TOR_OCCUPANCY.IA_MISS_CRD",
        "PerPkg": "1",
        "PublicDescription": "TOR Occupancy : CRds issued by iA Cores that Missed the LLC",
        "UMask": "0xc80ffe01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "TOR Occupancy for CRDs from local IA cores to locally homed memory",
        "Counter": "0",
        "EventCode": "0x36",
        "EventName": "UNC_CHA_TOR_OCCUPANCY.IA_MISS_CRD_LOCAL",
        "PerPkg": "1",
        "PublicDescription": "TOR Occupancy : CRd issued by iA Cores that Missed the LLC - HOMed locally",
        "UMask": "0xc80efe01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "TOR Occupancy for Code read prefetch from local IA that miss the cache",
        "Counter": "0",
        "EventCode": "0x36",
        "EventName": "UNC_CHA_TOR_OCCUPANCY.IA_MISS_CRD_PREF",
        "PerPkg": "1",
        "PublicDescription": "TOR Occupancy : CRd_Prefs issued by iA Cores that Missed the LLC",
        "UMask": "0xc88ffe01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "TOR Occupancy for CRD Prefetches from local IA cores to locally homed memory",
        "Counter": "0",
        "EventCode": "0x36",
        "EventName": "UNC_CHA_TOR_OCCUPANCY.IA_MISS_CRD_PREF_LOCAL",
        "PerPkg": "1",
        "PublicDescription": "TOR Occupancy : CRd_Prefs issued by iA Cores that Missed the LLC - HOMed locally",
        "UMask": "0xc88efe01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "TOR Occupancy for Data read opt from local IA that miss the cache",
        "Counter": "0",
        "EventCode": "0x36",
        "EventName": "UNC_CHA_TOR_OCCUPANCY.IA_MISS_DRD_OPT",
        "Experimental": "1",
        "PerPkg": "1",
        "PublicDescription": "TOR Occupancy : DRd_Opt issued by iA Cores that missed the LLC",
        "UMask": "0xc827fe01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "TOR Occupancy for Data read opt prefetch from local IA that miss the cache",
        "Counter": "0",
        "EventCode": "0x36",
        "EventName": "UNC_CHA_TOR_OCCUPANCY.IA_MISS_DRD_OPT_PREF",
        "Experimental": "1",
        "PerPkg": "1",
        "PublicDescription": "TOR Occupancy : DRd_Opt_Prefs issued by iA Cores that missed the LLC",
        "UMask": "0xc8a7fe01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "TOR Occupancy for ItoM requests from local IA cores that miss the cache",
        "Counter": "0",
        "EventCode": "0x36",
        "EventName": "UNC_CHA_TOR_OCCUPANCY.IA_MISS_ITOM",
        "PerPkg": "1",
        "PublicDescription": "TOR Occupancy : ItoMs issued by iA Cores that Missed LLC",
        "UMask": "0xcc47fe01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "TOR Occupancy for Last level cache prefetch code read from local IA that miss the cache",
        "Counter": "0",
        "EventCode": "0x36",
        "EventName": "UNC_CHA_TOR_OCCUPANCY.IA_MISS_LLCPREFCODE",
        "PerPkg": "1",
        "PublicDescription": "TOR Occupancy : LLCPrefCode issued by iA Cores that missed the LLC",
        "UMask": "0xcccffe01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "TOR Occupancy for Last level cache prefetch data read from local IA that miss the cache",
        "Counter": "0",
        "EventCode": "0x36",
        "EventName": "UNC_CHA_TOR_OCCUPANCY.IA_MISS_LLCPREFDATA",
        "PerPkg": "1",
        "PublicDescription": "TOR Occupancy : LLCPrefData issued by iA Cores that missed the LLC",
        "UMask": "0xccd7fe01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "TOR Occupancy for Last level cache prefetch read for ownership from local IA that miss the cache",
        "Counter": "0",
        "EventCode": "0x36",
        "EventName": "UNC_CHA_TOR_OCCUPANCY.IA_MISS_LLCPREFRFO",
        "PerPkg": "1",
        "PublicDescription": "TOR Occupancy : LLCPrefRFO issued by iA Cores that missed the LLC",
        "UMask": "0xccc7fe01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "TOR Occupancy for WCILF requests from local IA cores to locally homed DDR addresses that miss the cache",
        "Counter": "0",
        "EventCode": "0x36",
        "EventName": "UNC_CHA_TOR_OCCUPANCY.IA_MISS_LOCAL_WCILF_DDR",
        "PerPkg": "1",
        "PublicDescription": "TOR Occupancy : WCiLFs issued by iA Cores targeting DDR that missed the LLC - HOMed locally",
        "UMask": "0xc8668601",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "TOR Occupancy for WCIL requests from local IA cores to locally homed DDR addresses that miss the cache",
        "Counter": "0",
        "EventCode": "0x36",
        "EventName": "UNC_CHA_TOR_OCCUPANCY.IA_MISS_LOCAL_WCIL_DDR",
        "PerPkg": "1",
        "PublicDescription": "TOR Occupancy : WCiLs issued by iA Cores targeting DDR that missed the LLC - HOMed locally",
        "UMask": "0xc86e8601",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "TOR Occupancy for Read for ownership from local IA that miss the cache",
        "Counter": "0",
        "EventCode": "0x36",
        "EventName": "UNC_CHA_TOR_OCCUPANCY.IA_MISS_RFO",
        "PerPkg": "1",
        "PublicDescription": "TOR Occupancy : RFOs issued by iA Cores that Missed the LLC",
        "UMask": "0xc807fe01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "TOR Occupancy for Read for ownership from local IA that miss the cache",
        "Counter": "0",
        "EventCode": "0x36",
        "EventName": "UNC_CHA_TOR_OCCUPANCY.IA_MISS_RFO_LOCAL",
        "PerPkg": "1",
        "PublicDescription": "TOR Occupancy : RFOs issued by iA Cores that Missed the LLC - HOMed locally",
        "UMask": "0xc806fe01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "TOR Occupancy for Read for ownership prefetch from local IA that miss the cache",
        "Counter": "0",
        "EventCode": "0x36",
        "EventName": "UNC_CHA_TOR_OCCUPANCY.IA_MISS_RFO_PREF",
        "PerPkg": "1",
        "PublicDescription": "TOR Occupancy : RFO_Prefs issued by iA Cores that Missed the LLC",
        "UMask": "0xc887fe01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "TOR Occupancy for Read for ownership prefetch from local IA that miss the cache",
        "Counter": "0",
        "EventCode": "0x36",
        "EventName": "UNC_CHA_TOR_OCCUPANCY.IA_MISS_RFO_PREF_LOCAL",
        "PerPkg": "1",
        "PublicDescription": "TOR Occupancy : RFO_Prefs issued by iA Cores that Missed the LLC - HOMed locally",
        "UMask": "0xc886fe01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "TOR Occupancy for UCRDF requests from local IA cores that miss the cache",
        "Counter": "0",
        "EventCode": "0x36",
        "EventName": "UNC_CHA_TOR_OCCUPANCY.IA_MISS_UCRDF",
        "PerPkg": "1",
        "PublicDescription": "TOR Occupancy : UCRdFs issued by iA Cores that Missed LLC",
        "UMask": "0xc877de01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "TOR Occupancy for WCIL requests from a local IA core that miss the cache",
        "Counter": "0",
        "EventCode": "0x36",
        "EventName": "UNC_CHA_TOR_OCCUPANCY.IA_MISS_WCIL",
        "PerPkg": "1",
        "PublicDescription": "TOR Occupancy : WCiLs issued by iA Cores that Missed the LLC",
        "UMask": "0xc86ffe01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "TOR Occupancy for WCILF requests from local IA core that miss the cache",
        "Counter": "0",
        "EventCode": "0x36",
        "EventName": "UNC_CHA_TOR_OCCUPANCY.IA_MISS_WCILF",
        "PerPkg": "1",
        "PublicDescription": "TOR Occupancy : WCiLF issued by iA Cores that Missed the LLC",
        "UMask": "0xc867fe01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "TOR Occupancy for WCILF requests from local IA cores to DDR homed addresses which miss the cache",
        "Counter": "0",
        "EventCode": "0x36",
        "EventName": "UNC_CHA_TOR_OCCUPANCY.IA_MISS_WCILF_DDR",
        "PerPkg": "1",
        "PublicDescription": "TOR Occupancy : WCiLFs issued by iA Cores targeting DDR that missed the LLC",
        "UMask": "0xc8678601",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "TOR Occupancy for WCIL requests from local IA cores to DDR homed addresses which miss the cache",
        "Counter": "0",
        "EventCode": "0x36",
        "EventName": "UNC_CHA_TOR_OCCUPANCY.IA_MISS_WCIL_DDR",
        "PerPkg": "1",
        "PublicDescription": "TOR Occupancy : WCiLs issued by iA Cores targeting DDR that missed the LLC",
        "UMask": "0xc86f8601",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "TOR Occupancy for WIL requests from local IA cores that miss the cache",
        "Counter": "0",
        "EventCode": "0x36",
        "EventName": "UNC_CHA_TOR_OCCUPANCY.IA_MISS_WIL",
        "PerPkg": "1",
        "PublicDescription": "TOR Occupancy : WiLs issued by iA Cores that Missed LLC",
        "UMask": "0xc87fde01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "TOR Occupancy for Read for ownership from local IA that miss the cache",
        "Counter": "0",
        "EventCode": "0x36",
        "EventName": "UNC_CHA_TOR_OCCUPANCY.IA_RFO",
        "PerPkg": "1",
        "PublicDescription": "TOR Occupancy : RFOs issued by iA Cores",
        "UMask": "0xc807ff01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "TOR Occupancy for Read for ownership prefetch from local IA that miss the cache",
        "Counter": "0",
        "EventCode": "0x36",
        "EventName": "UNC_CHA_TOR_OCCUPANCY.IA_RFO_PREF",
        "PerPkg": "1",
        "PublicDescription": "TOR Occupancy : RFO_Prefs issued by iA Cores",
        "UMask": "0xc887ff01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "TOR Occupancy for SpecItoM events that are initiated from the Core",
        "Counter": "0",
        "EventCode": "0x36",
        "EventName": "UNC_CHA_TOR_OCCUPANCY.IA_SPECITOM",
        "PerPkg": "1",
        "PublicDescription": "TOR Occupancy : SpecItoMs issued by iA Cores",
        "UMask": "0xcc57ff01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "TOR Occupancy for WbMtoI requests from local IA cores",
        "Counter": "0",
        "EventCode": "0x36",
        "EventName": "UNC_CHA_TOR_OCCUPANCY.IA_WBMTOI",
        "PerPkg": "1",
        "PublicDescription": "TOR Occupancy : WbMtoIs issued by iA Cores",
        "UMask": "0xcc27ff01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "TOR Occupancy for WCIL requests from a local IA core",
        "Counter": "0",
        "EventCode": "0x36",
        "EventName": "UNC_CHA_TOR_OCCUPANCY.IA_WCIL",
        "PerPkg": "1",
        "PublicDescription": "TOR Occupancy : WCiLs issued by iA Cores",
        "UMask": "0xc86fff01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "TOR Occupancy for WCILF requests from local IA core",
        "Counter": "0",
        "EventCode": "0x36",
        "EventName": "UNC_CHA_TOR_OCCUPANCY.IA_WCILF",
        "PerPkg": "1",
        "PublicDescription": "TOR Occupancy : WCiLF issued by iA Cores",
        "UMask": "0xc867ff01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "TOR Occupancy for All TOR inserts from local IO devices",
        "Counter": "0",
        "EventCode": "0x36",
        "EventName": "UNC_CHA_TOR_OCCUPANCY.IO",
        "Experimental": "1",
        "PerPkg": "1",
        "PublicDescription": "TOR Occupancy : All requests from IO Devices",
        "UMask": "0xc001ff04",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "TOR Occupancy for CLFlush requests from IO devices",
        "Counter": "0",
        "EventCode": "0x36",
        "EventName": "UNC_CHA_TOR_OCCUPANCY.IO_CLFLUSH",
        "PerPkg": "1",
        "PublicDescription": "TOR Occupancy : CLFlushes issued by IO Devices",
        "UMask": "0xc8c3ff04",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "TOR Occupancy for All TOR inserts from local IO devices which hit the cache",
        "Counter": "0",
        "EventCode": "0x36",
        "EventName": "UNC_CHA_TOR_OCCUPANCY.IO_HIT",
        "Experimental": "1",
        "PerPkg": "1",
        "PublicDescription": "TOR Occupancy : All requests from IO Devices that hit the LLC",
        "UMask": "0xc001fd04",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "TOR Occupancy for ItoMs from local IO devices which hit the cache",
        "Counter": "0",
        "EventCode": "0x36",
        "EventName": "UNC_CHA_TOR_OCCUPANCY.IO_HIT_ITOM",
        "PerPkg": "1",
        "PublicDescription": "TOR Occupancy : ItoMs issued by IO Devices that Hit the LLC",
        "UMask": "0xcc43fd04",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "TOR Occupancy for ItoMCacheNears, indicating a partial write request, from IO Devices that hit the LLC",
        "Counter": "0",
        "EventCode": "0x36",
        "EventName": "UNC_CHA_TOR_OCCUPANCY.IO_HIT_ITOMCACHENEAR",
        "PerPkg": "1",
        "PublicDescription": "TOR Occupancy : ItoMCacheNears, indicating a partial write request, from IO Devices that hit the LLC",
        "UMask": "0xcd43fd04",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "TOR Occupancy for PCIRDCURs issued by IO devices which hit the LLC",
        "Counter": "0",
        "EventCode": "0x36",
        "EventName": "UNC_CHA_TOR_OCCUPANCY.IO_HIT_PCIRDCUR",
        "PerPkg": "1",
        "PublicDescription": "TOR Occupancy : PCIRdCurs issued by IO Devices that hit the LLC",
        "UMask": "0xc8f3fd04",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "TOR Occupancy for RFOs from local IO devices which hit the cache",
        "Counter": "0",
        "EventCode": "0x36",
        "EventName": "UNC_CHA_TOR_OCCUPANCY.IO_HIT_RFO",
        "PerPkg": "1",
        "PublicDescription": "TOR Occupancy : RFOs issued by IO Devices that hit the LLC",
        "UMask": "0xc803fd04",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "TOR Occupancy for All TOR ItoM inserts from local IO devices",
        "Counter": "0",
        "EventCode": "0x36",
        "EventName": "UNC_CHA_TOR_OCCUPANCY.IO_ITOM",
        "PerPkg": "1",
        "PublicDescription": "TOR Occupancy : ItoMs issued by IO Devices",
        "UMask": "0xcc43ff04",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "TOR Occupancy for ItoMCacheNears, indicating a partial write request, from IO Devices",
        "Counter": "0",
        "EventCode": "0x36",
        "EventName": "UNC_CHA_TOR_OCCUPANCY.IO_ITOMCACHENEAR",
        "PerPkg": "1",
        "PublicDescription": "TOR Occupancy : ItoMCacheNears, indicating a partial write request, from IO Devices",
        "UMask": "0xcd43ff04",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "TOR Occupancy for All TOR inserts from local IO devices which miss the cache",
        "Counter": "0",
        "EventCode": "0x36",
        "EventName": "UNC_CHA_TOR_OCCUPANCY.IO_MISS",
        "Experimental": "1",
        "PerPkg": "1",
        "PublicDescription": "TOR Occupancy : All requests from IO Devices that missed the LLC",
        "UMask": "0xc001fe04",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "TOR Occupancy for All TOR ItoM inserts from local IO devices which miss the cache",
        "Counter": "0",
        "EventCode": "0x36",
        "EventName": "UNC_CHA_TOR_OCCUPANCY.IO_MISS_ITOM",
        "PerPkg": "1",
        "PublicDescription": "TOR Occupancy : ItoMs issued by IO Devices that missed the LLC",
        "UMask": "0xcc43fe04",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "TOR Occupancy for ItoMCacheNears, indicating a partial write request, from IO Devices that missed the LLC",
        "Counter": "0",
        "EventCode": "0x36",
        "EventName": "UNC_CHA_TOR_OCCUPANCY.IO_MISS_ITOMCACHENEAR",
        "PerPkg": "1",
        "PublicDescription": "TOR Occupancy : ItoMCacheNears, indicating a partial write request, from IO Devices that missed the LLC",
        "UMask": "0xcd43fe04",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "TOR Occupancy for PCIRDCURs issued by IO devices which miss the LLC",
        "Counter": "0",
        "EventCode": "0x36",
        "EventName": "UNC_CHA_TOR_OCCUPANCY.IO_MISS_PCIRDCUR",
        "PerPkg": "1",
        "PublicDescription": "TOR Occupancy : PCIRdCurs issued by IO Devices that missed the LLC",
        "UMask": "0xc8f3fe04",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "TOR Occupancy for All TOR RFO inserts from local IO devices which miss the cache",
        "Counter": "0",
        "EventCode": "0x36",
        "EventName": "UNC_CHA_TOR_OCCUPANCY.IO_MISS_RFO",
        "PerPkg": "1",
        "PublicDescription": "TOR Occupancy : RFOs issued by IO Devices that missed the LLC",
        "UMask": "0xc803fe04",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "TOR Occupancy for PCIRDCURs issued by IO devices",
        "Counter": "0",
        "EventCode": "0x36",
        "EventName": "UNC_CHA_TOR_OCCUPANCY.IO_PCIRDCUR",
        "PerPkg": "1",
        "PublicDescription": "TOR Occupancy : PCIRdCurs issued by IO Devices",
        "UMask": "0xc8f3ff04",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "TOR Occupancy for RFOs from local IO devices",
        "Counter": "0",
        "EventCode": "0x36",
        "EventName": "UNC_CHA_TOR_OCCUPANCY.IO_RFO",
        "PerPkg": "1",
        "PublicDescription": "TOR Occupancy : RFOs issued by IO Devices",
        "UMask": "0xc803ff04",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "TOR Occupancy for WBMtoI requests from IO devices",
        "Counter": "0",
        "EventCode": "0x36",
        "EventName": "UNC_CHA_TOR_OCCUPANCY.IO_WBMTOI",
        "PerPkg": "1",
        "PublicDescription": "TOR Occupancy : WbMtoIs issued by IO Devices",
        "UMask": "0xcc23ff04",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "TOR Occupancy for All locally initiated requests",
        "Counter": "0",
        "EventCode": "0x36",
        "EventName": "UNC_CHA_TOR_OCCUPANCY.LOC_ALL",
        "Experimental": "1",
        "PerPkg": "1",
        "PublicDescription": "TOR Occupancy : All from Local iA and IO",
        "UMask": "0xc000ff05",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "TOR Occupancy for All from Local iA",
        "Counter": "0",
        "EventCode": "0x36",
        "EventName": "UNC_CHA_TOR_OCCUPANCY.LOC_IA",
        "Experimental": "1",
        "PerPkg": "1",
        "PublicDescription": "TOR Occupancy : All from Local iA",
        "UMask": "0xc000ff01",
        "Unit": "CHA"
    },
    {
        "BriefDescription": "TOR Occupancy for All from Local IO",
        "Counter": "0",
        "EventCode": "0x36",
        "EventName": "UNC_CHA_TOR_OCCUPANCY.LOC_IO",
        "Experimental": "1",
        "PerPkg": "1",
        "PublicDescription": "TOR Occupancy : All from Local IO",
        "UMask": "0xc000ff04",
        "Unit": "CHA"
    }
]
