//
//Copyright (c) 1996  Digital Equipment Corporation
//
//Permission is hereby granted, free of charge, to any person obtaining
//a copy of this software and associated documentation files (the
//"Software"), to deal in the Software without restriction, including
//without limitation the rights to use, copy, modify, merge, publish,
//distribute, sublicense, and sell copies of the Software, and to
//permit persons to whom the Software is furnished to do so, subject to
//the following conditions:
//
//The above copyright notice and this permission notice shall be included
//in all copies or substantial portions of the Software.
//
//THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND, EXPRESS
//OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF
//MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT.
//IN NO EVENT SHALL DIGITAL EQUIPMENT CORPORATION BE LIABLE FOR ANY CLAIM,
//DAMAGES OR OTHER LIABILITY, WHETHER IN AN ACTION OF CONTRACT, TORT OR
//OTHERWISE, ARISING FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR
//THE USE OR OTHER DEALINGS IN THE SOFTWARE.
//
//Except as contained in this notice, the name of the Digital Equipment
//Corporation shall not be used in advertising or otherwise to promote
//the sale, use or other dealings in this Software without prior written
//authorization from Digital Equipment Corporation.
//
// HISTORY
// Log
// Revision 1.2  1996/06/18  09:13:22  erik
// use flags correctly, assorted cleanups and consortium fixes
//
// Revision 1.1.6.2  1995/08/07  17:40:34  William_Walker
// 	Upgrade XKB to protocol 0.62 (dual submit from decx11)
// 	[1995/08/06  14:06:25  William_Walker]
//
// Revision 1.1.2.4  1995/08/05  15:25:55  William_Walker
// 	Upgrade to XKB protocol 0.62
// 	[1995/08/05  14:39:58  William_Walker]
//
// Revision 1.1.2.3  1995/06/27  12:17:31  William_Walker
// 	     Rename <TLDE> to ISO9995 compliant <AE00>.
// 	[1995/06/26  20:24:04  William_Walker]
//
// Revision 1.1.2.2  1995/06/05  19:21:28  William_Walker
// 	New file.  I love keymaps.
// 	[1995/06/05  18:07:29  William_Walker]
//
// EndLog
//
// @(#)RCSfile: lk  Revision: /main/3  (DEC) Date: 1996/01/24 12:13:31
//
xkb_keycodes "lk_common" {
    // "Function" keys
    <FK01>	= 86;
    <FK02>	= 87;
    <FK03>	= 88;
    <FK04>	= 89;
    <FK05>	= 90;
    <FK06>	= 100;
    <FK07>	= 101;
    <FK08>	= 102;
    <FK09>	= 103;
    <FK10>	= 104;
    <FK11>	= 113;
    <FK12>	= 114;

    <UP>	= 170;
    <LEFT>	= 167;
    <DOWN>	= 169;
    <RGHT>	= 168;

    // "Keypad" keys
    <KP7>	= 157;
    <KP8>	= 158;
    <KP9>	= 159;
    <KP4>	= 153;
    <KP5>	= 154;
    <KP6>	= 155;
    <KP1>	= 150;
    <KP2>	= 151;
    <KP3>	= 152;
    <KPEN>	= 149;
    <KP0>	= 146;
    <KPDL>	= 148;

    // "Alphanumeric" keys
    <AE00>	= 191;
    <AE01>	= 192;
    <AE02>	= 197;
    <AE03>	= 203;
    <AE04>	= 208;
    <AE05>	= 214;
    <AE06>	= 219;
    <AE07>	= 224;
    <AE08>	= 229;
    <AE09>	= 234;
    <AE10>	= 239;
    <AE11>	= 249;
    <AE12>	= 245;
    <BKSP>	= 188;

    <TAB>	= 190;
    <AD01>	= 193;
    <AD02>	= 198;
    <AD03>	= 204;
    <AD04>	= 209;
    <AD05>	= 215;
    <AD06>	= 220;
    <AD07>	= 225;
    <AD08>	= 230;
    <AD09>	= 235;
    <AD10>	= 240;
    <AD11>	= 250;
    <AD12>	= 246;
    <RTRN>	= 189;

    <LCTL>	= 175;
    <CAPS>	= 176;
    <AC01>	= 194;
    <AC02>	= 199;
    <AC03>	= 205;
    <AC04>	= 210;
    <AC05>	= 216;
    <AC06>	= 221;
    <AC07>	= 226;
    <AC08>	= 231;
    <AC09>	= 236;
    <AC10>	= 242;
    <AC11>	= 251;

    <LFSH>	= 174;
    <AB01>	= 195;
    <AB02>	= 200;
    <AB03>	= 206;
    <AB04>	= 211;
    <AB05>	= 217;
    <AB06>	= 222;
    <AB07>	= 227;
    <AB08>	= 232;
    <AB09>	= 237;
    <AB10>	= 243;
    <RTSH>	= 171;

    <SPCE>	= 212;

    <LDM>	= 255; // Support R5 Lock Down Modifiers

    alias <TLDE> = <AE00>;
};

xkb_keycodes "lkx01" {
    include "digital_vndr/lk(lk_common)"
    <AB00>	= 201;
    <FK13>	= 115;
    <FK14>	= 116;
    <FK17>	= 128;
    <FK18>	= 129;
    <FK19>	= 130;
    <FK20>	= 131;
    <HELP>	= 124;
    <DO>	= 125;
    <FIND>	= 138;
    <INS>	= 139;
    <DELE>	= 140;
    <SELE>	= 141;
    <PGUP>	= 142;
    <PGDN>	= 143;
    <KPF1>	= 161;
    <KPF2>	= 162;
    <KPF3>	= 163;
    <KPF4>	= 164;
    <KPSU>	= 160;
    <KPCO>	= 156;
    <BKSL>	= 247;
    <LCMP>	= 177;
};

xkb_keycodes "lk201" {
    include "digital_vndr/lk(lkx01)"
    indicator 4 = "Scroll Lock";
    indicator 3 = "Caps Lock";
    indicator 2 = "Compose";
    indicator 1 = "Wait";
};

xkb_keycodes "lk421" {
    include	"digital_vndr/lk(lkx01)"
    <LALT>	= 172;
    <RALT>	= 178;
    <RCMP>	= 173;
};

xkb_keycodes "lk401" {
    include	"digital_vndr/lk(lk421)"
    indicator 4 = "Scroll Lock";
    indicator 3 = "Caps Lock";
};

xkb_keycodes "lk44x" {
    include "digital_vndr/lk(lk_common)"
    <ESC>	= 85;
    <PRSC>	= 115;
    <SCLK>	= 116;
    <PAUS>	= 124;
    <INS>	= 138;
    <HOME>	= 139;
    <PGUP>	= 140;
    <DELE>	= 141;
    <END>	= 142;
    <PGDN>	= 143;
    <NMLK>	= 161;
    <KPDV>	= 162;
    <KPMU>	= 163;
    <KPSU>	= 164;
    <KPAD>	= 156;
    <LALT>	= 172;
    <RALT>	= 178;
    <RCTL>	= 173;
};

xkb_keycodes "lk443" {
    include "digital_vndr/lk(lk44x)"
    <BKSL>	= 247;
    indicator 3 = "Caps Lock";
    indicator 4 = "Scroll Lock";
    indicator 5 = "Num Lock";
};

xkb_keycodes "lk444" {
    include "digital_vndr/lk(lk44x)"
    <BKSL>	= 201;
    <AC12>	= 247;
    indicator 3 = "Caps Lock";
    indicator 4 = "Scroll Lock";
    indicator 5 = "Num Lock";
};

// LK201-LT = lk201
// LK421-AJ = lk421  +AB11
// LK421-JJ = lk421aj+MUHE+KANJ+HIRA
// LK401-AJ = lk401
// LK401-BJ = lk401  +MUHE+KANJ+HIRA
// LK401-JJ = lk401bj+AB11
// LK401-LT = lk401
// LK441-LT = lk443

xkb_keycodes "lk421aj" {
    include "digital_vndr/lk(lk421)"
    <AB11>  = 252;
};

xkb_keycodes "lk421jj" {
    include "digital_vndr/lk(lk421aj)"
    <MUHE>  = 94;
    <KANJ>  = 95;
    <HIRA>  = 97;
};

xkb_keycodes "lk401bj" {
    include "digital_vndr/lk(lk401)"
    <MUHE>  = 94;
    <KANJ>  = 95;
    <HIRA>  = 97;
};

xkb_keycodes "lk401jj" {
    include "digital_vndr/lk(lk401bj)"
    <AB11>  = 252;
};
