//
//Copyright (c) 1996  Digital Equipment Corporation
//
//Permission is hereby granted, free of charge, to any person obtaining
//a copy of this software and associated documentation files (the
//"Software"), to deal in the Software without restriction, including
//without limitation the rights to use, copy, modify, merge, publish,
//distribute, sublicense, and sell copies of the Software, and to
//permit persons to whom the Software is furnished to do so, subject to
//the following conditions:
//
//The above copyright notice and this permission notice shall be included
//in all copies or substantial portions of the Software.
//
//THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND, EXPRESS
//OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF
//MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT.
//IN NO EVENT SHALL DIGITAL EQUIPMENT CORPORATION BE LIABLE FOR ANY CLAIM,
//DAMAGES OR OTHER LIABILITY, WHETHER IN AN ACTION OF CONTRACT, TORT OR
//OTHERWISE, ARISING FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR
//THE USE OR OTHER DEALINGS IN THE SOFTWARE.
//
//Except as contained in this notice, the name of the Digital Equipment
//Corporation shall not be used in advertising or otherwise to promote
//the sale, use or other dealings in this Software without prior written
//authorization from Digital Equipment Corporation.
//
// HISTORY
// Log
// Revision 1.2  1996/06/18  09:13:25  erik
// use flags correctly, assorted cleanups and consortium fixes
//
// Revision 1.1.6.3  1995/10/25  21:00:14  William_Walker
// 	Add pc104-key support
// 	[1995/10/23  15:46:21  William_Walker]
//
// Revision 1.1.6.2  1995/08/07  17:40:37  William_Walker
// 	Upgrade XKB to protocol 0.62 (dual submit from decx11)
// 	[1995/08/06  14:06:28  William_Walker]
//
// Revision 1.1.2.4  1995/08/05  15:25:56  William_Walker
// 	Upgrade to XKB protocol 0.62
// 	[1995/08/05  14:40:02  William_Walker]
//
// Revision 1.1.2.3  1995/06/27  12:17:32  William_Walker
// 	     Rename <TLDE> to ISO9995 compliant <AE00>.
// 	[1995/06/26  20:24:07  William_Walker]
//
// Revision 1.1.2.2  1995/06/05  19:21:31  William_Walker
// 	New file.  I love keymaps.
// 	[1995/06/05  18:07:34  William_Walker]
//
// EndLog
//
// @(#)RCSfile: pc  Revision: /main/3  (DEC) Date: 1996/01/24 12:13:36
//
xkb_keycodes "pc_common" {
    // "Function" keys
    <FK01>	= 9;
    <FK02>	= 15;
    <FK03>	= 23;
    <FK04>	= 31;
    <FK05>	= 39;
    <FK06>	= 47;
    <FK07>	= 55;
    <FK08>	= 63;
    <FK09>	= 71;
    <FK10>	= 79;
    <FK11>	= 86;
    <FK12>	= 94;

    // "Editing" keys

    <UP>	= 99;
    <LEFT>	= 97;
    <DOWN>	= 96;
    <RGHT>	= 106;

    // "Keypad" keys
    <KP7>	= 108;
    <KP8>	= 117;
    <KP9>	= 125;

    <KP4>	= 107;
    <KP5>	= 115;
    <KP6>	= 116;

    <KP1>	= 105;
    <KP2>	= 114;
    <KP3>	= 122;
    <KPEN>	= 121;

    <KP0>	= 112;
    <KPDL>	= 113;

    // "Alphanumeric" keys
    <AE01>	= 22;
    <AE02>	= 30;
    <AE03>	= 38;
    <AE04>	= 37;
    <AE05>	= 46;
    <AE06>	= 54;
    <AE07>	= 61;
    <AE08>	= 62;
    <AE09>	= 70;
    <AE10>	= 69;
    <AE11>	= 78;
    <AE12>	= 85;
    <BKSP>	= 102;

    <TAB>	= 13;
    <AD01>	= 21;
    <AD02>	= 29;
    <AD03>	= 36;
    <AD04>	= 45;
    <AD05>	= 44;
    <AD06>	= 53;
    <AD07>	= 60;
    <AD08>	= 67;
    <AD09>	= 68;
    <AD10>	= 77;
    <AD11>	= 84;
    <AD12>	= 91;

    <CAPS>	= 20;
    <AC01>	= 28;
    <AC02>	= 27;
    <AC03>	= 35;
    <AC04>	= 43;
    <AC05>	= 52;
    <AC06>	= 51;
    <AC07>	= 59;
    <AC08>	= 66;
    <AC09>	= 75;
    <AC10>	= 76;
    <AC11>	= 82;
    <RTRN>	= 90;

    <LFSH>	= 18;
    <AB01>	= 26;
    <AB02>	= 34;
    <AB03>	= 33;
    <AB04>	= 42;
    <AB05>	= 50;
    <AB06>	= 49;
    <AB07>	= 58;
    <AB08>	= 65;
    <AB09>	= 73;
    <AB10>	= 74;
    <RTSH>	= 89;

    <LCTL>	= 17;
    <LALT>	= 25;
    <SPCE>	= 41;
    <RALT>	= 57;

    <LDM>	= 255; // Support R5 Lock Down Modifiers

};

xkb_keycodes "pc10x" {
    include "digital_vndr/pc(pc_common)"
    <ESC>	= 8;
    <AE00>	= 14;
    <PRSC>	= 87;
    <SCLK>	= 95;
    <PAUS>	= 98;
    <INS>	= 103;
    <HOME>	= 110;
    <PGUP>	= 111;
    <DELE>	= 100;
    <END>	= 101;
    <PGDN>	= 109;
    <NMLK>	= 118;
    <KPDV>	= 119;
    <KPMU>	= 126;
    <KPSU>	= 132;
    <KPAD>	= 124;
    <RCTL>	= 88;

    alias <TLDE> = <AE00>;

    indicator 3 = "Caps Lock";
    indicator 4 = "Scroll Lock";
};

xkb_keycodes "pc101" {
    include "digital_vndr/pc(pc10x)"
    <BKSL>  = 92;
    indicator 5 = "Num Lock";
};


xkb_keycodes "pc102" {
    include "digital_vndr/pc(pc10x)"
    <BKSL>  = 19;
    <AC12>  = 83;
    indicator 5 = "Num Lock";
};

xkb_keycodes "pc104" {
    include "digital_vndr/pc(pc101)"
    <LWIN>  = 139;
    <RWIN>  = 140;
    <MENU>  = 141;
};

xkb_keycodes "lk411_common" {
    include "digital_vndr/pc(pc_common)"
    <AE00>      = 8;
    <AB00>      = 14;
    <FK13>	= 24;
    <FK14>	= 10;
    <FK17>	= 16;
    <FK18>	= 87;
    <FK19>	= 95;
    <FK20>	= 98;
    <HELP>	= 11;
    <DO>	= 12;
    <FIND>	= 110;
    <INS>	= 103;
    <DELE>	= 100;
    <SELE>	= 101;
    <PGUP>	= 111;
    <PGDN>	= 109;
    <KPF1>	= 118;
    <KPF2>	= 119;
    <KPF3>	= 126;
    <KPF4>	= 132;
    <KPSU>	= 19;
    <KPCO>	= 124;
    <LCMP>	= 40;
    <RCMP>	= 88;

    alias <TLDE> = <AE00>;

    indicator 3 = "Caps Lock";
    indicator 4 = "Scroll Lock";
};

xkb_keycodes "lk411" {
    include "digital_vndr/pc(lk411_common)"
    <BKSL>	= 92;
};

xkb_keycodes "lk450" {
    include	"digital_vndr/pc(lk411)"
    indicator 2 = "Compose";
    indicator 1 = "Wait";
};

// Japanese variants
//
// PCXAJ-AA = pc+BKSL+AC12+AB11+MUHE+KANJ+HIRA+indicator
// LK411-AJ = lk411+MUHE+KANJ+HIRA
// LK411-JJ = lk411+BKSL+AZ01+MUHE+KANJ+HIRA
// LK411-LT = lk411

xkb_keycodes "pcxajaa" {
    include "digital_vndr/pc(pc10x)"
    <BKSL>  = 93;
    <AC12>  = 83;
    <AB11>  = 81;
    <MUHE>  = 133;
    <KANJ>  = 134;
    <HIRA>  = 135;
    indicator 5 = "Group 2";
};

xkb_keycodes "lk411jj" {
    include "digital_vndr/pc(lk411_common)"
    <AB11>  = 81;
    <BKSL>  = 83;
    <MUHE>  = 133;
    <KANJ>  = 134;
    <HIRA>  = 135;
};
