ommits â€”
  all additions are new enum values, table entries, and small functions
- "Tested-by: Sean Rhodes" from Star Labs confirms hardware validation

**YES**

 sound/hda/codecs/realtek/alc269.c | 25 +++++++++++++++++++++++++
 1 file changed, 25 insertions(+)

diff --git a/sound/hda/codecs/realtek/alc269.c b/sound/hda/codecs/realtek/alc269.c
index 36053042ca772..9f64bb97c3f9a 100644
--- a/sound/hda/codecs/realtek/alc269.c
+++ b/sound/hda/codecs/realtek/alc269.c
@@ -1017,6 +1017,24 @@ static int alc269_resume(struct hda_codec *codec)
 	return 0;
 }
 
+#define STARLABS_STARFIGHTER_SHUTUP_DELAY_MS	30
+
+static void starlabs_starfighter_shutup(struct hda_codec *codec)
+{
+	if (snd_hda_gen_shutup_speakers(codec))
+		msleep(STARLABS_STARFIGHTER_SHUTUP_DELAY_MS);
+}
+
+static void alc233_fixup_starlabs_starfighter(struct hda_codec *codec,
+					      const struct hda_fixup *fix,
+					      int action)
+{
+	struct alc_spec *spec = codec->spec;
+
+	if (action == HDA_FIXUP_ACT_PRE_PROBE)
+		spec->shutup = starlabs_starfighter_shutup;
+}
+
 static void alc269_fixup_pincfg_no_hp_to_lineout(struct hda_codec *codec,
 						 const struct hda_fixup *fix, int action)
 {
@@ -4040,6 +4058,7 @@ enum {
 	ALC245_FIXUP_CLEVO_NOISY_MIC,
 	ALC269_FIXUP_VAIO_VJFH52_MIC_NO_PRESENCE,
 	ALC233_FIXUP_MEDION_MTL_SPK,
+	ALC233_FIXUP_STARLABS_STARFIGHTER,
 	ALC294_FIXUP_BASS_SPEAKER_15,
 	ALC283_FIXUP_DELL_HP_RESUME,
 	ALC294_FIXUP_ASUS_CS35L41_SPI_2,
@@ -6499,6 +6518,10 @@ static const struct hda_fixup alc269_fixups[] = {
 			{ }
 		},
 	},
+	[ALC233_FIXUP_STARLABS_STARFIGHTER] = {
+		.type = HDA_FIXUP_FUNC,
+		.v.func = alc233_fixup_starlabs_starfighter,
+	},
 	[ALC294_FIXUP_BASS_SPEAKER_15] = {
 		.type = HDA_FIXUP_FUNC,
 		.v.func = alc294_fixup_bass_speaker_15,
@@ -7651,6 +7674,7 @@ static const struct hda_quirk alc269_fixup_tbl[] = {
 	SND_PCI_QUIRK(0x2782, 0x1705, "MEDION E15433", ALC269VC_FIXUP_INFINIX_Y4_MAX),
 	SND_PCI_QUIRK(0x2782, 0x1707, "Vaio VJFE-ADL", ALC298_FIXUP_SPK_VOLUME),
 	SND_PCI_QUIRK(0x2782, 0x4900, "MEDION E15443", ALC233_FIXUP_MEDION_MTL_SPK),
+	SND_PCI_QUIRK(0x7017, 0x2014, "Star Labs StarFighter", ALC233_FIXUP_STARLABS_STARFIGHTER),
 	SND_PCI_QUIRK(0x8086, 0x2074, "Intel NUC 8", ALC233_FIXUP_INTEL_NUC8_DMIC),
 	SND_PCI_QUIRK(0x8086, 0x2080, "Intel NUC 8 Rugged", ALC256_FIXUP_INTEL_NUC8_RUGGED),
 	SND_PCI_QUIRK(0x8086, 0x2081, "Intel NUC 10", ALC256_FIXUP_INTEL_NUC10),
@@ -7747,6 +7771,7 @@ static const struct hda_model_fixup alc269_fixup_models[] = {
 	{.id = ALC298_FIXUP_TPT470_DOCK_FIX, .name = "tpt470-dock-fix"},
 	{.id = ALC298_FIXUP_TPT470_DOCK, .name = "tpt470-dock"},
 	{.id = ALC233_FIXUP_LENOVO_MULTI_CODECS, .name = "dual-codecs"},
+	{.id = ALC233_FIXUP_STARLABS_STARFIGHTER, .name = "starlabs-starfighter"},
 	{.id = ALC700_FIXUP_INTEL_REFERENCE, .name = "alc700-ref"},
 	{.id = ALC269_FIXUP_SONY_VAIO, .name = "vaio"},
 	{.id = ALC269_FIXUP_DELL_M101Z, .name = "dell-m101z"},
-- 
2.51.0[PATCH AUTOSEL 6.19-6.12] ALSA: hda/realtek: Fix speaker pop on Star Labs StarFighterSasha Levin <sashal@kernel.org> undefinedpatches@lists.linux.dev, stable@vger.kernel.org undefined undefined undefined undefined undefined undefined undefined undefined¦}†Â<
