{
  "schema_version": "1.4.0",
  "id": "GHSA-79c2-28c3-2cp6",
  "modified": "2025-04-11T04:11:44Z",
  "published": "2022-05-17T01:32:42Z",
  "aliases": [
    "CVE-2013-4784"
  ],
  "details": "The HP Integrated Lights-Out (iLO) BMC implementation allows remote attackers to bypass authentication and execute arbitrary IPMI commands by using cipher suite 0 (aka cipher zero) and an arbitrary password.",
  "severity": [],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2013-4784"
    },
    {
      "type": "WEB",
      "url": "https://exchange.xforce.ibmcloud.com/vulnerabilities/85569"
    },
    {
      "type": "WEB",
      "url": "https://lists.gnu.org/archive/html/freeipmi-devel/2013-02/msg00013.html"
    },
    {
      "type": "WEB",
      "url": "http://fish2.com/ipmi/cipherzero.html"
    },
    {
      "type": "WEB",
      "url": "http://osvdb.org/show/osvdb/93040"
    },
    {
      "type": "WEB",
      "url": "http://www.metasploit.com/modules/auxiliary/scanner/ipmi/ipmi_cipher_zero"
    },
    {
      "type": "WEB",
      "url": "http://www.oracle.com/technetwork/topics/security/cpujan2015-1972971.html"
    },
    {
      "type": "WEB",
      "url": "http://www.wired.com/threatlevel/2013/07/ipmi"
    }
  ],
  "database_specific": {
    "cwe_ids": [
      "CWE-287"
    ],
    "severity": "HIGH",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2013-07-08T22:55:00Z"
  }
}